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CABLE & WIRE FOR ELECTRICAL, ELV AND INDUSTRIAL PROJECTS
H03VV-F Light Duty PVC Flexible Cord
Exact model: H03VV-F
PRODUCT IMAGES
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	H03VV-F · Primary



PRODUCT OVERVIEW
NexPro H03VV-F Light Duty PVC Flexible Cord is supplied as a configurable pvc flexible cord product family. Catalog models are preserved exactly as H03VV-F. Use the source-derived tables below to select the required conductor construction, core arrangement, cross-section and dimensions.
	Product line
	Cable & Wire for Electrical, ELV and Industrial Projects

	Series / family
	PVC flexible cord

	Exact model
	H03VV-F

	Applications
	Equipment connections, Flexible wiring, OEM electrical assemblies


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Cable category
	Catalog model
	Configuration

	H03VV-F
	H03VV-F Light Duty PVC Flexible Cord
	PVC flexible cord
	H03VV-F
	Select from source table


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Cable category
	PVC flexible cord

	Catalog model
	H03VV-F

	Configuration
	Select from source table

	Manufacturer models
	H03VV-F

	2x0,5
	Resistance at 20 °C
(Ohm/km): 39 | External Diameter (mm): 4,75 | Weight (kg/km): 40 | Class: Eca

	2x0,75
	Resistance at 20 °C
(Ohm/km): 26 | External Diameter (mm): 5,20 | Weight (kg/km): 41 | Class: Eca

	3G0,5
	Resistance at 20 °C
(Ohm/km): 39 | External Diameter (mm): 5,25 | Weight (kg/km): 42 | Class: Eca

	3G0,75
	Resistance at 20 °C
(Ohm/km): 26 | External Diameter (mm): 5,50 | Weight (kg/km): 49 | Class: Eca

	4x0,5
	Resistance at 20 °C
(Ohm/km): 39 | External Diameter (mm): 5,60 | Weight (kg/km): 47 | Class: Eca

	4x0,75
	Resistance at 20 °C
(Ohm/km): 26 | External Diameter (mm): 6,30 | Weight (kg/km): 64 | Class: Eca


ENGINEERING TABLES
H03VV-F · Source Specification Table 1
	Section (mm²)
	Resistance at 20 °C (Ohm/km)
	External Diameter (mm)
	Weight (kg/km)
	Class

	2x0,5
	39
	4,75
	40
	Eca

	2x0,75
	26
	5,20
	41
	Eca

	3G0,5
	39
	5,25
	42
	Eca

	3G0,75
	26
	5,50
	49
	Eca

	4x0,5
	39
	5,60
	47
	Eca

	4x0,75
	26
	6,30
	64
	Eca


H03VV-F · Source Specification Table 2
	1. Conductor
	Flexible electrolytic copper conductor (Class V) according to BS EN 60228:2005 (previously BS6360) and UNE 60228.

	2. Insulation
	PVC insulation type TI-2 according to BS7655, UNE-EN 50363-3 and EN 50363-3

	3. Sheath
	PVC sheath type TM-2 according to BS7655, UNE-EN 50363-4-1 and EN 50363-4-1

	Nominal voltage
	300/300 V

	Test voltage
	2.000 V A.C.

	Maximum temperature
	70 °C

	Other characteristics
	—

	Colours according to UNE 21089 and HD 303S2 (colour marking when less than five conductors) and UNE-EN 50334 and EN 50334 (inscription marking when more than five conductors)Non-flame propagating according to UNE-EN 60332-1-2, EN 60332-1-2 and IEC 60332-1-2PVC with reduced hydrogen chloride (HCI) emissionCPR Classification according to EN 50575
	—



	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
	Page 1


image2.png




image3.jpg




image1.png








