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CABLE & WIRE FOR ELECTRICAL, ELV AND INDUSTRIAL PROJECTS
SPT-1 / SPT-2 / SPT-3 Lamp Cord
Exact model: SPT-1 | SPT-2 | SPT-3
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PRODUCT OVERVIEW
NexPro SPT-1 / SPT-2 / SPT-3 Lamp Cord is supplied as a configurable lamp cord product family. Catalog models are preserved exactly as SPT-1, SPT-2, SPT-3. Use the source-derived tables below to select the required conductor construction, core arrangement, cross-section and dimensions.
	Product line
	Cable & Wire for Electrical, ELV and Industrial Projects

	Series / family
	Lamp cord

	Exact model
	SPT-1 | SPT-2 | SPT-3

	Applications
	Equipment connections, Flexible wiring, OEM electrical assemblies


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Cable category
	Catalog model
	Configuration

	SPT-1 | SPT-2 | SPT-3
	SPT-1 / SPT-2 / SPT-3 Lamp Cord
	Lamp cord
	SPT-1 | SPT-2 | SPT-3
	Select from source table


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Cable category
	Lamp cord

	Catalog model
	SPT-1 | SPT-2 | SPT-3

	Configuration
	Select from source table

	Manufacturer models
	SPT-1 / SPT-2 / SPT-3

	SPT - 1
	Size
(AWG): — | No. of Conductors: — | Conductor Stranding (No./AWG): — | Insulation Thickness (inches): — | Overall Diameter (inches): — | Ampacity (amps): — | Weight (lbs/kft): —

	SPT1-18/2
	Size
(AWG): 18 | No. of Conductors: 2 | Conductor Stranding (No./AWG): 41/34 | Insulation Thickness (inches): 0.030 | Overall Diameter (inches): 0.11 x 0.22 | Ampacity (amps): 10 | Weight (lbs/kft): 20

	SPT1-18/3
	Size
(AWG): 18 | No. of Conductors: 3 | Conductor Stranding (No./AWG): 41/34 | Insulation Thickness (inches): 0.030 | Overall Diameter (inches): 0.11 x 0.33 | Ampacity (amps): 10 | Weight (lbs/kft): 30

	SPT – 2
	Size
(AWG): — | No. of Conductors: — | Conductor Stranding (No./AWG): — | Insulation Thickness (inches): — | Overall Diameter (inches): — | Ampacity (amps): — | Weight (lbs/kft): —

	SPT2-18/2
	Size
(AWG): 18 | No. of Conductors: 2 | Conductor Stranding (No./AWG): 41/34 | Insulation Thickness (inches): 0.045 | Overall Diameter (inches): 0.14 x 0.27 | Ampacity (amps): 10 | Weight (lbs/kft): 27

	SPT2-16/2
	Size
(AWG): 16 | No. of Conductors: 2 | Conductor Stranding (No./AWG): 65/34 | Insulation Thickness (inches): 0.045 | Overall Diameter (inches): 0.15 x 0.30 | Ampacity (amps): 13 | Weight (lbs/kft): 36

	SPT2-16/3
	Size
(AWG): 16 | No. of Conductors: 3 | Conductor Stranding (No./AWG): 65/34 | Insulation Thickness (inches): 0.045 | Overall Diameter (inches): 0.15 x 0.45 | Ampacity (amps): 10 | Weight (lbs/kft): 54

	SPT – 3
	Size
(AWG): — | No. of Conductors: — | Conductor Stranding (No./AWG): — | Insulation Thickness (inches): — | Overall Diameter (inches): — | Ampacity (amps): — | Weight (lbs/kft): —


ENGINEERING TABLES
SPT-1 | SPT-2 | SPT-3 · Source Specification Table 1
	Part Number
	Size (AWG)
	No. of Conductors
	Conductor Stranding (No./AWG)
	Insulation Thickness (inches)
	Overall Diameter (inches)
	Ampacity (amps)
	Weight (lbs/kft)

	SPT - 1
	—
	—
	—
	—
	—
	—
	—

	SPT1-18/2
	18
	2
	41/34
	0.030
	0.11 x 0.22
	10
	20

	SPT1-18/3
	18
	3
	41/34
	0.030
	0.11 x 0.33
	10
	30

	SPT – 2
	—
	—
	—
	—
	—
	—
	—

	SPT2-18/2
	18
	2
	41/34
	0.045
	0.14 x 0.27
	10
	27

	SPT2-16/2
	16
	2
	65/34
	0.045
	0.15 x 0.30
	13
	36

	SPT2-16/3
	16
	3
	65/34
	0.045
	0.15 x 0.45
	10
	54

	SPT – 3
	—
	—
	—
	—
	—
	—
	—

	SPT3-16/2
	16
	2
	65/34
	0.060
	0.18 x 0.36
	13
	47

	SPT3-14/2
	14
	2
	41/30
	0.060
	0.20 x 0.40
	18
	61

	SPT3-14/3
	14
	3
	41/30
	0.060
	0.20 x 0.60
	15
	92

	SPT3-12/2
	12
	2
	65/30
	0.060
	0.22 x 0.44
	25
	82

	SPT3-12/3
	12
	3
	65/30
	0.060
	0.22 x 0.66
	20
	123
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