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	PRODUCT SPECIFICATION
Low-voltage power cable
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CABLE & WIRE FOR ELECTRICAL, ELV AND INDUSTRIAL PROJECTS
VV PVC Insulated PVC Sheathed Power Cable
Exact model: VV
PRODUCT IMAGES
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	VV · Primary



PRODUCT OVERVIEW
NexPro VV PVC Insulated PVC Sheathed Power Cable is supplied as a configurable low-voltage power cable product family. Catalog models are preserved exactly as VV. Use the source-derived tables below to select the required conductor construction, core arrangement, cross-section and dimensions.
	Product line
	Cable & Wire for Electrical, ELV and Industrial Projects

	Series / family
	Low-voltage power cable

	Exact model
	VV

	Applications
	Low-voltage distribution, Industrial power projects, Fixed and buried installations


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Cable category
	Catalog model
	Configuration

	VV
	VV PVC Insulated PVC Sheathed Power Cable
	Low-voltage power cable
	VV
	Select from source table


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Cable category
	Low-voltage power cable

	Catalog model
	VV

	Configuration
	Select from source table

	Manufacturer models
	VV

	Specification status
	No numeric source table was published for this product family

	Selection guidance
	Confirm the exact model, voltage rating, conductor or core configuration, cross-section, installation conditions, required length and applicable project requirements in the RFQ.


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Low-voltage distribution
Industrial power projects
Fixed and buried installations
	Confirm conductor material and construction, core count and cross-section.
Confirm voltage/model, installation method and environmental conditions.
Confirm required length, drum or coil packing, quantity and destination requirements.


Project supply: MOQ — Confirm by cable type, size and length · Lead time — Confirm after specification review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	VV

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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