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BS 6004 624-Y Twin and Earth PVC Cable
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CABLE & WIRE FOR ELECTRICAL, ELV AND INDUSTRIAL PROJECTS
BS 6004 624-Y Twin and Earth PVC Cable
Models: 624-Y | NYM-J | NYM-O
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PRODUCT OVERVIEW
NexPro BS 6004 624-Y Twin and Earth PVC Cable is supplied as a configurable fixed installation cable product family. Catalog models are preserved exactly as 624-Y. Use the source-derived tables below to select the required conductor construction, core arrangement, cross-section and dimensions.
	Product line
	Cable & Wire for Electrical, ELV and Industrial Projects

	Series / family
	Fixed installation cable

	Exact model
	624-Y | NYM-J | NYM-O

	Applications
	Building wiring, Electrical panels, Fixed installation projects


MODEL COMPARISON
	Exact model
	Product / variant
	Cable category
	Catalog model
	Configuration

	624-Y
	BS 6004 624-Y Twin and Earth PVC Cable
	Fixed installation cable
	624-Y
	Select from source table

	NYM-J | NYM-O
	NYM-J / NYM-O PVC Installation Cable
	Fixed installation cable
	NYM-J | NYM-O
	Select from source table


TECHNICAL SPECIFICATIONS
	Parameter
	624-Y
	NYM-J | NYM-O

	Cable category
	Fixed installation cable
	Fixed installation cable

	Catalog model
	624-Y
	NYM-J | NYM-O

	Configuration
	Select from source table
	Select from source table

	Manufacturer models
	624-Y
	NYM-J / NYM-O

	Specification status
	No numeric source table was published for this product family
	Not provided

	Selection guidance
	Confirm the exact model, voltage rating, conductor or core configuration, cross-section, installation conditions, required length and applicable project requirements in the RFQ.
	Not provided

	2 x 1.5 RE
	Not provided
	Specified value: 12.1 | Value 2: 0.42 | Value 3: 8.8 | Value 4: 115 | Value 5: 100 R, 500 Sp

	3 x 1.5 RE
	Not provided
	Specified value: 12.1 | Value 2: 0.44 | Value 3: 8.5 | Value 4: 120 | Value 5: 100 R, 500 Sp

	4 x 1.5 RE
	Not provided
	Specified value: 12.1 | Value 2: 0.53 | Value 3: 9.3 | Value 4: 145 | Value 5: 100 R, 500 Sp

	5 x 1.5 RE
	Not provided
	Specified value: 12.1 | Value 2: 0.58 | Value 3: 10.2 | Value 4: 170 | Value 5: 100 R, 500 Sp

	7 x 1.5 RE
	Not provided
	Specified value: 12.1 | Value 2: 0.67 | Value 3: 12.3 | Value 4: 235 | Value 5: 1000 D

	10 x 1.5 RE
	Not provided
	Specified value: 12.1 | Value 2: 1.05 | Value 3: 14.3 | Value 4: 330 | Value 5: 500 Sp, 1000 Sp

	12 x 1.5 RE
	Not provided
	Specified value: 12.1 | Value 2: 1.17 | Value 3: 14.4 | Value 4: 400 | Value 5: 100 R, 500 Sp

	3 x 2.5 RE
	Not provided
	Specified value: 7.41 | Value 2: 0.58 | Value 3: 9.9 | Value 4: 165 | Value 5: 100 R, 500 Sp


ENGINEERING TABLES
NYM-J | NYM-O · NYM-J or -O
	Parameter
	Specified value
	Value 2
	Value 3
	Value 4
	Value 5

	2 x 1.5 RE
	12.1
	0.42
	8.8
	115
	100 R, 500 Sp

	3 x 1.5 RE
	12.1
	0.44
	8.5
	120
	100 R, 500 Sp

	4 x 1.5 RE
	12.1
	0.53
	9.3
	145
	100 R, 500 Sp

	5 x 1.5 RE
	12.1
	0.58
	10.2
	170
	100 R, 500 Sp

	7 x 1.5 RE
	12.1
	0.67
	12.3
	235
	1000 D

	10 x 1.5 RE
	12.1
	1.05
	14.3
	330
	500 Sp, 1000 Sp

	12 x 1.5 RE
	12.1
	1.17
	14.4
	400
	100 R, 500 Sp

	3 x 2.5 RE
	7.41
	0.58
	9.9
	165
	100 R, 500 Sp

	4 x 2.5 RE
	7.41
	0.67
	10.7
	205
	100 R, 500 Sp

	5 x 2.5 RE
	7.41
	0.72
	11.7
	245
	100 R, 500 Sp

	7 x 2.5 RE
	7.41
	0.88
	14.5
	335
	1000 D

	3 x 4 RE
	4.61
	0.72
	10.8
	265
	1000 D

	4 x 4 RE
	4.61
	0.92
	12.8
	305
	1000 D

	5 x 4 RE
	4.61
	1.11
	13.9
	370
	1000 D

	5 x 6 RE
	3.08
	1.28
	15.1
	460
	1000 D
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