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	PRODUCT SPECIFICATION
H05V-U / H07V-U PVC Insulated Solid Building Wire
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CABLE & WIRE FOR ELECTRICAL, ELV AND INDUSTRIAL PROJECTS
H05V-U / H07V-U PVC Insulated Solid Building Wire
Models: H05V-U | H07V-U | H05V-R | H07V-R
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	H05V-U | H07V-U · Primary
	H05V-R | H07V-R · Primary



PRODUCT OVERVIEW
NexPro H05V-U / H07V-U PVC Insulated Solid Building Wire is supplied as a configurable single-core building wire product family. Catalog models are preserved exactly as H05V-U, H07V-U. Use the source-derived tables below to select the required conductor construction, core arrangement, cross-section and dimensions.
	Product line
	Cable & Wire for Electrical, ELV and Industrial Projects

	Series / family
	Single-core building wire

	Exact model
	H05V-U | H07V-U | H05V-R | H07V-R

	Applications
	Building wiring, Electrical panels, Fixed installation projects


MODEL COMPARISON
	Exact model
	Product / variant
	Cable category
	Catalog model
	Configuration

	H05V-U | H07V-U
	H05V-U / H07V-U PVC Insulated Solid Building Wire
	Single-core building wire
	H05V-U | H07V-U
	Select from source table

	H05V-R | H07V-R
	H05V-R / H07V-R PVC Insulated Stranded Building Wire
	Single-core building wire
	H05V-R | H07V-R
	Select from source table


TECHNICAL SPECIFICATIONS
	Parameter
	H05V-U | H07V-U
	H05V-R | H07V-R

	Cable category
	Single-core building wire
	Single-core building wire

	Catalog model
	H05V-U | H07V-U
	H05V-R | H07V-R

	Configuration
	Select from source table
	Select from source table

	Manufacturer models
	H05V-U / H07V-U
	H05V-R / H07V-R

	Conductor
	Specified value: Bare solid copper
	Not provided

	Insulation
	Specified value: PVC
	Not provided

	Minimum bending radius, fixed installation
	Specified value: 4xOD
	Not provided

	Colour
	Specified value: According to EN 50525-1
	Not provided

	Specification status
	Not provided
	No numeric source table was published for this product family

	Selection guidance
	Not provided
	Confirm the exact model, voltage rating, conductor or core configuration, cross-section, installation conditions, required length and applicable project requirements in the RFQ.


ENGINEERING TABLES
H05V-U | H07V-U · Construction
	Parameter
	Specified value

	Conductor
	Bare solid copper

	Insulation
	PVC

	Minimum bending radius, fixed installation
	4xOD

	Colour
	According to EN 50525-1


H05V-U | H07V-U · Source Specification Table 2
	Type Code
	Cross-section [mm]
	Nominal Outer Diameter [mm]
	Current rating, installation in open air, ambient 30°C [A]
	Total weight [kg/km]

	H05V-U
	0,5
	2,0
	12
	9

	H05V-U
	0,75
	2,2
	15
	11

	H05V-U
	1
	2,3
	19
	14

	H07V-U
	1,5
	2,8
	24
	20

	H07V-U
	2,5
	3,4
	32
	31

	H07V-U
	4
	3,8
	42
	46

	H07V-U
	6
	4,3
	54
	68

	H07V-U
	10
	5,4
	73
	111
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