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	PRODUCT SPECIFICATION
H05Z-R / H07Z-R LSZH Insulated Wire
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CABLE & WIRE FOR ELECTRICAL, ELV AND INDUSTRIAL PROJECTS
H05Z-R / H07Z-R LSZH Insulated Wire
Models: H05Z-R | H07Z-R | H07Z1-U
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	H05Z-R | H07Z-R · Primary
	H07Z1-U · Primary



PRODUCT OVERVIEW
NexPro H05Z-R / H07Z-R LSZH Insulated Wire is supplied as a configurable low-smoke zero-halogen wire product family. Catalog models are preserved exactly as H05Z-R, H07Z-R. Use the source-derived tables below to select the required conductor construction, core arrangement, cross-section and dimensions.
	Product line
	Cable & Wire for Electrical, ELV and Industrial Projects

	Series / family
	Low-smoke zero-halogen wire

	Exact model
	H05Z-R | H07Z-R | H07Z1-U

	Applications
	Public buildings, Emergency circuits, Low-smoke installation projects


MODEL COMPARISON
	Exact model
	Product / variant
	Cable category
	Catalog model
	Configuration

	H05Z-R | H07Z-R
	H05Z-R / H07Z-R LSZH Insulated Wire
	Low-smoke zero-halogen wire
	H05Z-R | H07Z-R
	Select from source table

	H07Z1-U
	H07Z1-U LSZH Solid Building Wire
	Low-smoke zero-halogen wire
	H07Z1-U
	Select from source table


TECHNICAL SPECIFICATIONS
	Parameter
	H05Z-R | H07Z-R
	H07Z1-U

	Cable category
	Low-smoke zero-halogen wire
	Low-smoke zero-halogen wire

	Catalog model
	H05Z-R | H07Z-R
	H07Z1-U

	Configuration
	Select from source table
	Select from source table

	Manufacturer models
	H05Z-R / H07Z-R
	H07Z1-U

	Specification status
	No numeric source table was published for this product family
	Not provided

	Selection guidance
	Confirm the exact model, voltage rating, conductor or core configuration, cross-section, installation conditions, required length and applicable project requirements in the RFQ.
	Not provided

	1.5
	Not provided
	Nominal Thickness of insulation
(mm): 0.7 | MAX. Resistance of conductor at 70°C (MΩ): 0.011 | Nom. outer diam. (mm): 2.6-3.2 | Approx. weight (kg/km): 21

	2.5
	Not provided
	Nominal Thickness of insulation
(mm): 0.8 | MAX. Resistance of conductor at 70°C (MΩ): 0.010 | Nom. outer diam. (mm): 3.2-3.9 | Approx. weight (kg/km): 35

	4
	Not provided
	Nominal Thickness of insulation
(mm): 0.8 | MAX. Resistance of conductor at 70°C (MΩ): 0.0087 | Nom. outer diam. (mm): 3.6-4.4 | Approx. weight (kg/km): 44

	6
	Not provided
	Nominal Thickness of insulation
(mm): 0.8 | MAX. Resistance of conductor at 70°C (MΩ): 0.0074 | Nom. outer diam. (mm): 4.1-5.0 | Approx. weight (kg/km): 66


ENGINEERING TABLES
H07Z1-U · Source Specification Table 1
	Cross section (mm²)
	Nominal Thickness of insulation (mm)
	MAX. Resistance of conductor at 70°C (MΩ)
	Nom. outer diam. (mm)
	Approx. weight (kg/km)

	1.5
	0.7
	0.011
	2.6-3.2
	21

	2.5
	0.8
	0.010
	3.2-3.9
	35

	4
	0.8
	0.0087
	3.6-4.4
	44

	6
	0.8
	0.0074
	4.1-5.0
	66
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