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CCTV & SURVEILLANCE SYSTEM
9013 Series
Models: NexPro-BL9013D3-4MP-TRI | NexPro-BL9013Y51-4MP-TRI | NexPro-BL9013M55-5MP-TRI
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PRODUCT OVERVIEW
4MP full-color, triode lamp, 24 LEDs (1W), built-in mic, 4000V surge protection
	Product line
	CCTV & Surveillance System

	Series / family
	9013

	Exact model
	NexPro-BL9013D3-4MP-TRI | NexPro-BL9013Y51-4MP-TRI | NexPro-BL9013M55-5MP-TRI

	Applications
	Harsh Environment, Critical Perimeter, Industrial


MODEL COMPARISON
	Exact model
	Product / variant
	Resolution
	Lens
	Illuminator

	NexPro-BL9013D3-4MP-TRI
	NexPro 4MP Premium Bullet (Triode, 24-LED, Audio)
	4MP
	F1.4 5MP fixed
	24-LED triode (1W)

	NexPro-BL9013Y51-4MP-TRI
	NexPro 4MP Premium Bullet (5MP Sensor, Triode, 24-LED, Audio)
	4MP (5MP sensor)
	F1.4 5MP fixed
	24-LED triode (1W)

	NexPro-BL9013M55-5MP-TRI
	NexPro 5MP Premium Bullet (Triode, 24-LED, Audio)
	5MP
	F1.4 5MP fixed
	24-LED triode (1W)


TECHNICAL SPECIFICATIONS
	Parameter
	NexPro-BL9013D3-4MP-TRI
	NexPro-BL9013Y51-4MP-TRI
	NexPro-BL9013M55-5MP-TRI

	Resolution
	4MP (2560×1440) @ real-time
	4MP
(5MP sensor); 4MP (2560×1440) @ real-time (5MP sensor for superior low-light performance)
	5MP (2592×1944) @ real-time

	Lens
	F1.4 5MP fixed lens
	F1.4 5MP fixed lens
	F1.4 5MP fixed lens

	Illuminator
	24-LED triode
(1W); 24-LED dual light (12×20mil IR + 12×1W warm white)
	24-LED triode
(1W); 24-LED dual light (12×20mil IR + 12×1W warm white)
	24-LED triode
(1W); 24-LED dual light (12×20mil IR + 12×1W warm white)

	Camera Type
	4MP Full-Color Network Bullet Camera (9013 Premium Housing)
	4MP Full-Color Network Bullet Camera
(5MP Sensor, 9013 Housing)
	5MP Full-Color Network Bullet Camera (9013 Premium Housing)

	Solution
	Tianview TR38Y33
	Tianview TB38Y51
	Tianview TB38M55

	Image Sensor
	1/2.7″ 4MP CMOS, low illumination
	1/2.7″ 5MP CMOS, low illumination
	1/2.7″ 5MP CMOS, low illumination

	Lamp Board
	Triode circuit design
	Triode circuit design
	Triode circuit design

	Audio
	Built-in microphone
	Built-in microphone
	Built-in microphone

	Protection
	Metal front cover, 4000V lightning surge protection
	Metal front cover, 4000V lightning surge protection
	Metal front cover, 4000V lightning surge protection

	Light Control
	3 switchable modes
	3 switchable modes
	3 switchable modes

	Quotation Type
	Bulk project quotation
	Bulk project quotation
	Bulk project quotation

	OEM/ODM
	Available for selected orders
	Available for selected orders
	Available for selected orders

	Documents
	Datasheet and installation reference
	Datasheet and installation reference
	Datasheet and installation reference

	Category
	CCTV System
	CCTV System
	CCTV System


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Harsh Environment
Critical Perimeter
Industrial
Logistics Hub
Mission-Critical Perimeter
Industrial Campus
Oil & Gas
	Confirm the exact model and required configuration.
Confirm quantity, destination, packing, branding, and documentation requirements.


Project supply: MOQ — Confirm by project quantity · Lead time — Confirm by project list · FOB port — China main ports · OEM/ODM — Available; confirm project scope
PROJECT CONFIGURATION CHECKLIST
	Exact model
	NexPro-BL9013D3-4MP-TRI

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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