
	[image: ]
	PRODUCT SPECIFICATION
106 Series


[image: ]
CCTV & SURVEILLANCE SYSTEM
106 Series
Models: NexPro-DM106D3-4MP-DIC | NexPro-DM106D3-4MP-DIC-DJ | NexPro-DM106MQ5-5MP-DIC-DJ
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PRODUCT OVERVIEW
4MP full-color, dual-IC, 8 LEDs, built-in mic, 4000V surge protection
	Product line
	CCTV & Surveillance System

	Series / family
	106

	Exact model
	NexPro-DM106D3-4MP-DIC | NexPro-DM106D3-4MP-DIC-DJ | NexPro-DM106MQ5-5MP-DIC-DJ

	Applications
	Indoor Corridor, Retail, Office


MODEL COMPARISON
	Exact model
	Product / variant
	Resolution
	Lens
	Illuminator

	NexPro-DM106D3-4MP-DIC
	NexPro 4MP Compact Dual-Light Dome (8-LED, Built-in Mic)
	4MP
	F1.4 5MP fixed
	8-LED dual light

	NexPro-DM106D3-4MP-DIC-DJ
	NexPro 4MP Compact Dual-Light Dome (8-LED, Two-Way Audio)
	4MP (5MP sensor)
	F1.4 5MP fixed
	8-LED dual light

	NexPro-DM106MQ5-5MP-DIC-DJ
	NexPro 5MP Premium Compact Dual-Light Dome (8-LED, Two-Way Audio)
	5MP
	F1.4 5MP fixed
	8-LED dual light


TECHNICAL SPECIFICATIONS
	Parameter
	NexPro-DM106D3-4MP-DIC
	NexPro-DM106D3-4MP-DIC-DJ
	NexPro-DM106MQ5-5MP-DIC-DJ

	Resolution
	4MP (2560×1440) @ real-time
	4MP (5MP sensor); 4MP (2560×1440) @ real-time
	5MP (2592×1944) @ real-time

	Lens
	F1.4 5MP fixed lens
	F1.4 5MP fixed lens
	F1.4 5MP fixed lens

	Illuminator
	8-LED dual light (4×20mil IR + 4×0.5W warm white)
	8-LED dual light (4×20mil IR + 4×0.5W warm white)
	8-LED dual light (4×20mil IR + 4×0.5W warm white)

	Camera Type
	4MP Full-Color Dual-Light Network Dome Camera (106 Series)
	4MP Full-Color Dual-Light Network Dome Camera with Two-Way Audio
(106 Series)
	5MP Premium Full-Color Dual-Light Network Dome Camera with Two-Way Audio
(106 Series)

	Solution
	Tianview TR38Y33
	Tianview TB38Y51 (5MP sensor, output 4MP)
	Tianview TB38M55

	Image Sensor
	1/2.7″ 4MP CMOS, low illumination
	1/2.7″ 5MP CMOS, low illumination
	1/2.7″ 5MP CMOS, low illumination

	Lamp Board
	Dual IC circuit design
	Dual IC circuit design
	Dual IC circuit design

	Audio
	Built-in microphone
	Built-in microphone and speaker (two-way audio)
	Built-in microphone and speaker (two-way audio)

	Protection
	Metal front cover, front heat dissipation, 4000V surge protection
	Metal front cover, front heat dissipation, 4000V surge protection
	Metal front cover, front heat dissipation, 4000V surge protection

	Light Control
	3 switchable modes
	3 switchable modes
	3 switchable modes

	Quotation Type
	Bulk project quotation
	Bulk project quotation
	Bulk project quotation

	OEM/ODM
	Available for selected orders
	Available for selected orders
	Available for selected orders

	Documents
	Datasheet and installation reference
	Datasheet and installation reference
	Datasheet and installation reference

	Category
	CCTV System
	CCTV System
	CCTV System


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Indoor Corridor
Retail
Office
Retail Counter
Indoor Premium Area
Office Lobby
	Confirm the exact model and required configuration.
Confirm quantity, destination, packing, branding, and documentation requirements.


Project supply: MOQ — Confirm by project quantity · Lead time — Confirm by project list · FOB port — China main ports · OEM/ODM — Available; confirm project scope
PROJECT CONFIGURATION CHECKLIST
	Exact model
	NexPro-DM106D3-4MP-DIC

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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