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RACK KVM & REMOTE CONSOLE MANAGEMENT
SP1708-C 8-port local VGA KVM (1920 × 1080)
Exact model: SP1708-C
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PRODUCT OVERVIEW
8-port local VGA KVM consoles for rack server management.
	Product line
	Rack KVM & Remote Console Management

	Series / family
	kvm-1708

	Exact model
	SP1708-C

	Applications
	Local server management, Data-room racks, Maintenance consoles


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Port Count
	Resolution
	Dimensions

	SP1708-C
	SP1708-C 8-port local VGA KVM (1920 × 1080)
	8
	1920 × 1080
	485 × 480 × 44 mm


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Port Count
	8

	Resolution
	1920 × 1080

	Dimensions
	485 × 480 × 44 mm

	Maximum Cascade Capacity
	Up to 256 devices
Source catalog wording:  “connections 256”

	I/O Interface
	PS/2 / USB dual-interface converter module

	Scan Interval
	1–255 seconds

	System Compatibility
	Windows, Vista, Linux, etc.

	Power Input
	A C100-240V, 50-60Hz, 1 A

	Power Consumption
	120V at 23 W; 230V at 25 W

	Operating Temperature
	0-40℃

	Storage Temperature
	-20-60℃

	Humidity
	0-80%RH, non-condensing

	Warranty
	3 years for main unit; 1 year for display

	Product series
	SP1708 8-Port Local VGA KVM Series

	Product category
	KVM


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Local server management
Data-room racks
Maintenance consoles
	Confirm the application, rack or room position, destination-market interface and mounting requirement.
Confirm electrical, network, accessory or protection scope from the product family and project drawings.
Confirm quantity, labeling, packing and required documents before purchase order.


Project supply: MOQ — Confirm by model and project quantity · Lead time — Confirm after configuration review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	SP1708-C

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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