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RACK KVM & REMOTE CONSOLE MANAGEMENT
SP8732 32-Port CAT5 Network KVM
Exact model: SP8732
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PRODUCT OVERVIEW
CAT5/IP KVM consoles for high-density server management and cascading.
	Product line
	Rack KVM & Remote Console Management

	Series / family
	kvm-cat5

	Exact model
	SP8732

	Applications
	High-density server racks, CAT5 KVM extension, Data center operations


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Port Connection
	Port Count
	Input / Output

	SP8732
	SP8732 32-Port CAT5 Network KVM
	RJ45
	32
	PS/2 / USB dual-interface converter module


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Port Connection
	RJ45

	Port Count
	32

	Input / Output
	PS/2 / USB dual-interface converter module

	Resolution
	1280 × 1024

	Scan Interval
	5–255 seconds

	Supported Systems
	Windows, Vista, Linux, etc.

	Power Input
	A C100-240V, 50-60Hz, 1 A

	Power Consumption
	120V at 23 W; 230V at 25 W

	Optional Modules
	CAT5 module or IP remote-access card module

	Host Interface
	USB / PS/2

	Cascading
	Supports bus and tree topologies

	Dimensions
	485 × 570 × 44 mm

	Warranty
	3 years for main unit; 1 year for display

	Product series
	32-Port CAT5/IP KVM Series

	Product category
	KVM


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	High-density server racks
CAT5 KVM extension
Data center operations
	Confirm the application, rack or room position, destination-market interface and mounting requirement.
Confirm electrical, network, accessory or protection scope from the product family and project drawings.
Confirm quantity, labeling, packing and required documents before purchase order.


Project supply: MOQ — Confirm by model and project quantity · Lead time — Confirm after configuration review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	SP8732

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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