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RACK PDU & POWER DISTRIBUTION
SP5071 Circuit Breaker & Overload Protection PDU
Exact model: SP5071
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PRODUCT OVERVIEW
2 documented configurations are consolidated on this product-group page so buyers can compare specifications without duplicate catalog cards.
	Product line
	Rack PDU & Power Distribution

	Series / family
	pdu-breaker

	Exact model
	SP5071

	Applications
	Server and network racks, Equipment cabinets, Overload-protected distribution


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Configurations
	Input Current
	Input Cable

	SP5071
	SP5071 Circuit Breaker & Overload Protection PDU
	2
	16 A
	3 m, 2.5 mm²


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Configurations
	2

	Input Current
	16 A

	Input Cable
	3 m, 2.5 mm²

	Function Module
	Circuit breaker

	Output
	7 × 16 A Chinese-standard outlets

	Rated Load
	4000 W

	Dimensions
	485 × 44.5 × 44.5 mm

	Input Plug
	16A Chinese-standard plug

	Product series
	Circuit Breaker & Overload Protection PDU Series

	Entity type
	Product group with selectable configurations


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Server and network racks
Equipment cabinets
Overload-protected distribution
	Confirm the application, rack or room position, destination-market interface and mounting requirement.
Confirm electrical, network, accessory or protection scope from the product family and project drawings.
Confirm quantity, labeling, packing and required documents before purchase order.


Project supply: MOQ — Confirm by model and project quantity · Lead time — Confirm after configuration review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	SP5071

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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