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RACK PDU & POWER DISTRIBUTION
Circuit Breaker & Overload Protection PDU Series
Models: DT7188 | SP5071 | SP51103 | SP5188 | SP6081
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PRODUCT OVERVIEW
Rack power distribution with circuit-breaker or overload-protection modules for enhanced overcurrent protection.
	Product line
	Rack PDU & Power Distribution

	Series / family
	pdu-breaker

	Exact model
	DT7188 | SP5071 | SP51103 | SP5188 | SP6081

	Applications
	Server and network racks, Equipment cabinets, Overload-protected distribution


MODEL COMPARISON
	Exact model
	Product / variant
	Input Current
	Input Cable
	Input Plug

	DT7188
	DT7188 10 A Switched Overload-Protected PDU
	10 A
	3 m, 1.5 mm²
	10A Chinese-standard plug

	SP5071
	SP5071 Circuit Breaker & Overload Protection PDU
	16 A
	3 m, 2.5 mm²
	Not provided

	SP51103
	SP51103 10-Outlet 3-in-1 Protection PDU
	16 A
	3 m, 2.5 mm²
	16A Chinese-standard plug

	SP5188
	SP5188 16 A Switched Overload-Protected PDU
	16 A
	3 m, 2.5 mm²
	16A Chinese-standard plug

	SP6081
	SP6081 32 A High-Power Circuit-Breaker PDU
	32 A
	Not provided
	Not provided


TECHNICAL SPECIFICATIONS
Models: DT7188 | SP5071 | SP51103 | SP5188
	Parameter
	DT7188
	SP5071
	SP51103
	SP5188

	Input Current
	10 A
	16 A
	16 A
	16 A

	Input Cable
	3 m, 1.5 mm²
	3 m, 2.5 mm²
	3 m, 2.5 mm²
	3 m, 2.5 mm²

	Input Plug — Key Specifications
	10A Chinese-standard plug
	Not provided
	16A Chinese-standard plug
	16A Chinese-standard plug

	Function Module
	Switch + overload protection
	Circuit breaker
	3-in-1 protection
	Switch + overload protection

	Output
	8 × 10 A universal outlets
	7 × 16 A Chinese-standard outlets
	10 × 10 A universal outlets
	8 × 10 A universal outlets

	Rated Load
	2500 W
	4000 W
	4000 W
	4000 W

	Dimensions
	485 × 44.5 × 44.5 mm
	485 × 44.5 × 44.5 mm
	485 × 44.5 × 44.5 mm
	485 × 44.5 × 44.5 mm

	Product series
	Circuit Breaker & Overload Protection PDU Series
	Circuit Breaker & Overload Protection PDU Series
	Circuit Breaker & Overload Protection PDU Series
	Circuit Breaker & Overload Protection PDU Series

	Product category
	PDU
	Not provided
	PDU
	PDU

	Configurations
	Not provided
	2
	Not provided
	Not provided

	Input Plug — Source Technical Data
	Not provided
	16A Chinese-standard plug
	Not provided
	Not provided

	Entity type
	Not provided
	Product group with selectable configurations
	Not provided
	Not provided


Models: SP6081
	Parameter
	Specification

	Cable Specification
	3 × 4 mm²

	Input Current
	32 A

	Rated Load
	6000 W

	Input Plug
	32A industrial plug

	Function Module
	Circuit breaker

	Output
	8 × 16 A Chinese-standard outlets

	Dimensions
	485 × 44.5 × 44.5 mm

	Product series
	Circuit Breaker & Overload Protection PDU Series

	Product category
	PDU


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Server and network racks
Equipment cabinets
Overload-protected distribution
	Confirm the application, rack or room position, destination-market interface and mounting requirement.
Confirm electrical, network, accessory or protection scope from the product family and project drawings.
Confirm quantity, labeling, packing and required documents before purchase order.


Project supply: MOQ — Confirm by model and project quantity · Lead time — Confirm after configuration review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	DT7188

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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