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RACK PDU & POWER DISTRIBUTION
Surge-Protected Rack PDU Series
Models: SP1182-2 | SP3182 | SP5082 | SP5087 | SP5182 | SP61202
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PRODUCT OVERVIEW
Rack power distribution with integrated surge protection for 10 A, 16 A and 32 A input configurations.
	Product line
	Rack PDU & Power Distribution

	Series / family
	pdu-spd

	Exact model
	SP1182-2 | SP3182 | SP5082 | SP5087 | SP5182 | SP61202

	Applications
	Network racks, Security cabinets, Surge-protected equipment distribution


MODEL COMPARISON
	Exact model
	Product / variant
	Input Current
	Input Cable
	Input Plug

	SP1182-2
	SP1182-2 Single-Row 1U High-Power PDU
	32 A
	Not provided
	Not provided

	SP3182
	SP3182 10 A SPDsurge-protected PDU
	10 A
	3 m, 1.5 mm²
	10A Chinese-standard plug

	SP5082
	SP5082 Surge-Protected Rack PDU
	16 A
	3 m, 2.5 mm²
	Not provided

	SP5087
	SP5087 16 A Switched Surge-Protected PDU
	16 A
	3 m, 2.5 mm²
	16A Chinese-standard plug

	SP5182
	SP5182 10 A SPDsurge-protected PDU
	10 A
	Not provided
	Not provided

	SP61202
	SP61202 20-Outlet Long-Form High-Power Surge-Protected PDU
	32 A
	Not provided
	Not provided


TECHNICAL SPECIFICATIONS
Models: SP1182-2 | SP3182 | SP5082 | SP5087
	Parameter
	SP1182-2
	SP3182
	SP5082
	SP5087

	Input Current
	32 A
	10 A
	16 A
	16 A

	Function Module — Key Specifications
	catalog states “hot plug lighting protection”
	Not provided
	Not provided
	Not provided

	Output — Key Specifications
	8 × 10 A universal outlets
	Not provided
	Not provided
	Not provided

	Rated Load
	8000 W
	2500 W
	4000 W
	4000 W

	Dimensions
	485 × 44.5 × 44.5 mm
	485 × 44.5 × 44.5 mm
	485 × 44.5 × 44.5 mm
	485 × 44.5 × 44.5 mm

	Product series
	Surge-Protected Rack PDU Series
	Surge-Protected Rack PDU Series
	Surge-Protected Rack PDU Series
	Surge-Protected Rack PDU Series

	Product category
	PDU
	PDU
	Not provided
	PDU

	Input Cable
	Not provided
	3 m, 1.5 mm²
	3 m, 2.5 mm²
	3 m, 2.5 mm²

	Input Plug — Key Specifications
	Not provided
	10A Chinese-standard plug
	Not provided
	16A Chinese-standard plug

	Function Module — Source Technical Data
	Not provided
	SPD protection
	SPD surge protection
	Switch + surge protection

	Output — Source Technical Data
	Not provided
	8 × 10 A universal outlets
	8 × 16 A Chinese-standard outlets
	8 × 16 A Chinese-standard outlets

	Configurations
	Not provided
	Not provided
	2
	Not provided

	Input Plug — Source Technical Data
	Not provided
	Not provided
	16A Chinese-standard plug
	Not provided

	Entity type
	Not provided
	Not provided
	Product group with selectable configurations
	Not provided


Models: SP5182 | SP61202
	Parameter
	SP5182
	SP61202

	Cable Specification
	3 × 1.5 mm²
	3 × 6 mm²

	Input Current
	10 A
	32 A

	Rated Load
	2500 W
	8000 W

	Input Plug
	10A Chinese-standard plug
	32A industrial plug

	Function Module
	SPD surge protection
	SPD surge protection

	Output
	8 × 10 A universal outlets
	20 × 10 A universal outlets

	Dimensions
	485 × 44.5 × 44.5 mm
	990 × 62 × 44.5 mm

	Product series
	Surge-Protected Rack PDU Series
	Surge-Protected Rack PDU Series

	Product category
	PDU
	PDU


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Network racks
Security cabinets
Surge-protected equipment distribution
	Confirm the application, rack or room position, destination-market interface and mounting requirement.
Confirm electrical, network, accessory or protection scope from the product family and project drawings.
Confirm quantity, labeling, packing and required documents before purchase order.


Project supply: MOQ — Confirm by model and project quantity · Lead time — Confirm after configuration review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	SP1182-2

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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