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RACK CABINETS & DATA CENTER CONTAINMENT
K1 Network & Server Cabinet Series
Models: K1-5006 | K1-5012 | K1-6042 | K1-6638 | K1-6642
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PRODUCT OVERVIEW
19-inch network and server cabinets for standard IT, networking and security equipment.
	Product line
	Rack Cabinets & Data Center Containment

	Series / family
	k1

	Exact model
	K1-5006 | K1-5012 | K1-6042 | K1-6638 | K1-6642

	Applications
	Wall-mount network cabinets, CCTV and ELV equipment racks, Small server rooms


MODEL COMPARISON
	Exact model
	Product / variant
	Type
	Dimensions
	Height

	K1-5006
	K1-5006 6U wall-mount network cabinet
	Network cabinet / wall-mount cabinet
	350 × 550 × 400 mm
	6U

	K1-5012
	K1-5012 12U Compact Network Cabinet
	Network cabinet
	450 × 550 × 700 mm
	12U

	K1-6042
	K1-6042 42U K1 server cabinet
	Server cabinet
	600 × 1000 × 2000 mm
	42U

	K1-6638
	K1-6638 38U K1 network cabinet
	Network cabinet
	600 × 600 × 1800 mm
	38U

	K1-6642
	K1-6642 42U K1 Cabinet (Duplicate Catalog Specification)
	Catalog classification: server cabinet
	catalog states 600 × 1000 × 2000 mm
	Not provided


TECHNICAL SPECIFICATIONS
Models: K1-5006 | K1-5012 | K1-6042 | K1-6638
	Parameter
	K1-5006
	K1-5012
	K1-6042
	K1-6638

	Type
	Network cabinet / wall-mount cabinet
	Network cabinet
	Server cabinet
	Network cabinet

	Dimensions
	350 × 550 × 400 mm
	450 × 550 × 700 mm
	600 × 1000 × 2000 mm
	600 × 600 × 1800 mm

	Height
	6U
	12U
	42U
	38U

	Mounting Rail Spacing
	485 mm (19-inch standard)
	485 mm (19-inch standard)
	485 mm (19-inch standard)
	485 mm (19-inch standard)

	Sheet Thickness
	mounting rails 2.0 mm; other panels 1.0 mm
	mounting rails 2.0 mm; other panels 1.0 mm
	mounting rails 2.0 mm; other / main load-bearing beam approx. 1.1±0.1 mm
	mounting rails 2.0 mm; other panels 1.1 mm

	Material / Finish
	SPCC cold-rolled steel, degreased and powder-coated
	SPCC cold-rolled steel, degreased and powder-coated
	SPCC cold-rolled steel, degreased and powder-coated
	SPCC cold-rolled steel, degreased and powder-coated

	Series Load Capacity
	Wall-mount small-cabinet load rating: ≤50 kg
	Small-cabinet catalog load rating: ≤50 kg
	K1 series catalog load rating: ≤600 kg
	≤600kg

	Standard Configuration
	cage nuts and screws × 20、6Umounting rails × 4、glass door × 1、side panels × 2
	cage nuts and screws × 20、12Umounting rails × 4、glass door × 1、side panels × 2、shelves × 1、casters × 4
	PDU × 1、cage nuts and screws × 20、M12leveling feet × 4、42Umounting rails × 4、front and rear mesh doors × 1、side panels × 2、fans × 2、shelves × 3、casters × 4
	PDU × 1、cage nuts and screws × 20、M12leveling feet × 4、38Umounting rails × 4、front and rear mesh doors × 1、side panels × 2、fans × 1、shelves × 3、casters × 4

	Recommended Equipment Depth
	<300 mm
	<350 mm
	<850 mm
	<450 mm

	Product series
	K1 Network & Server Cabinet Series
	K1 Network & Server Cabinet Series
	K1 Network & Server Cabinet Series
	K1 Network & Server Cabinet Series

	Product category
	Data Center Cabinet
	Data Center Cabinet
	Data Center Cabinet
	Data Center Cabinet


Models: K1-6642
	Parameter
	Specification

	Type
	Catalog classification: server cabinet

	Dimensions
	catalog states 600 × 1000 × 2000 mm

	Mounting Rail Spacing
	485 mm (19-inch standard)

	Sheet Thickness
	mounting rails 2.0 mm; main load-bearing beam approx. 1.1±0.1 mm

	Material / Finish
	SPCC cold-rolled steel, degreased and powder-coated

	Standard Configuration
	Same catalog specification as K1-6042

	Recommended Equipment Depth
	<850 mm

	Product series
	K1 Network & Server Cabinet Series

	Product category
	Data Center Cabinet


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Wall-mount network cabinets
CCTV and ELV equipment racks
Small server rooms
	Confirm the application, rack or room position, destination-market interface and mounting requirement.
Confirm electrical, network, accessory or protection scope from the product family and project drawings.
Confirm quantity, labeling, packing and required documents before purchase order.


Project supply: MOQ — Confirm by model and project quantity · Lead time — Confirm after configuration review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	K1-5006

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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