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SMART LOCK & ELECTRONIC ACCESS HARDWARE
NX-HL-2031E Series
Models: NX-HL-2031E | NX-HL-2031E-V65
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	NX-HL-2031E · Primary
	NX-HL-2031E-V65 · Primary



PRODUCT OVERVIEW
A card, mechanical key smart door lock. Designed for residential, apartment, commercial building applications.
	Product line
	Smart Lock & Electronic Access Hardware

	Series / family
	Hotel Electronic Locks

	Exact model
	NX-HL-2031E | NX-HL-2031E-V65

	Applications
	Residential, Apartment, Commercial Building


MODEL COMPARISON
	Exact model
	Product / variant
	Product family
	Access
	Application

	NX-HL-2031E
	NexPro IC Card Hotel Lock NX-HL-2031E
	Hotel Lock Systems
	IC Card / Mechanical Key
	Residential

	NX-HL-2031E-V65
	NexPro IC Card Hotel Lock NX-HL-2031E-V65
	Hotel Lock Systems
	IC Card / Mechanical Key
	Residential


TECHNICAL SPECIFICATIONS
	Parameter
	NX-HL-2031E
	NX-HL-2031E-V65

	Product family
	Hotel Lock Systems
	Hotel Lock Systems

	Access
	IC Card / Mechanical Key
	IC Card / Mechanical Key

	Application
	Residential
	Residential

	Chip
	Texas Instruments TI Instrument Chip
	Texas Instruments TI Instrument Chip

	Card specs
	ATMEL Temic induction card
	ATMEL Temic induction card

	Production process
	Sheet metal insertion on PVC surface
	Sheet metal insertion on PVC surface

	System logic
	Conflict prevention mechanism
	Conflict prevention mechanism

	Card reading
	Non-contact induction type
	Non-contact induction type

	Read/write
	Read, write, and encrypt
	Read, write, and encrypt

	Opening time
	Press handle once after door opening; 7 seconds auto-lock
	Press handle once after door opening; 7 seconds auto-lock

	Unlock record
	Store latest unlock record in lock loop
	Store latest unlock record in lock loop

	Applicable scope
	Special lock for anti-theft doors, suitable for family, apartments, office buildings
	Special lock for anti-theft doors, suitable for family, apartments, office buildings

	Working voltage
	6A / 4 knots high energy alkaline battery V
	6A / 4 knots high energy alkaline battery V

	Static power consumption
	< 30 microamperes
	< 30 microamperes

	Dynamic power consumption
	Approximately 200 amps mA
	Approximately 200 amps mA

	Undervoltage index
	Below 4.8V still able to unlock >200 times
	Below 4.8V still able to unlock >200 times

	Battery life
	Normal continuous opening over 10000 times
	Normal continuous opening over 10000 times

	Storage capacity
	32 bytes
	32 bytes

	Installation
	Conventional side strip 24x240 / 30x240, customized
	Conventional side strip 24x240 / 30x240, customized

	Series
	Hotel Electronic Locks
	Hotel Electronic Locks

	Quotation type
	Project and bulk quotation
	Project and bulk quotation

	OEM/ODM
	Confirm branding, finish, packaging and software scope
	Confirm branding, finish, packaging and software scope



	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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