
	[image: ]
	PRODUCT SPECIFICATION
Standalone model


[image: ]
UPS UNINTERRUPTIBLE POWER SUPPLY
AL-WM Wall-Mounted LiFePO4 Batteries
Exact model: AL-WM-WALL-BATTERY
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PRODUCT OVERVIEW
AL-WM Wall-Mounted LiFePO4 Batteries with 4 source-reviewed models for Residential storage, inverter battery banks and DC backup systems. Model configuration and destination-market requirements are confirmed during RFQ review.
	Product line
	UPS Uninterruptible Power Supply

	Series / family
	Standalone model

	Exact model
	AL-WM-WALL-BATTERY

	Applications
	Residential storage, inverter battery banks and DC backup systems


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Topology
	Power Range
	Phase

	AL-WM-WALL-BATTERY
	AL-WM Wall-Mounted LiFePO4 Batteries
	Wall-mounted LiFePO4 battery
	10KWH to 26KWH
	DC charge input / DC discharge output


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Topology
	Wall-mounted LiFePO4 battery

	Power Range
	10KWH to 26KWH

	Phase
	DC charge input / DC discharge output

	Form Factor
	Wall mounted

	Waveform
	DC

	Power Factor
	Model-specific; confirm on quotation

	Battery Types
	Source-defined lithium or LiFePO4 configuration

	SKU
	AL-WM-WALL-BATTERY

	Available Configurations
	AL-WM512200; AL-WM512300; AL-WM512346; AL-WM512519

	Exact Configuration
	Confirm one listed configuration during RFQ review

	Destination Requirements
	To be confirmed


ENGINEERING TABLES
AL-WM-WALL-BATTERY · Complete Model Specifications — AL-WM512200 | AL-WM512300 | AL-WM512346 | AL-WM512519
	Parameter
	AL-WM512200
	AL-WM512300
	AL-WM512346
	AL-WM512519

	Rated capacity
	10KWH
	15KWH
	18KWH
	26KWH

	Battery configuration
	51.2V 200Ah / 10kWh
	51.2V 300Ah / 15kWh
	51.2V 346Ah / 18kWh
	51.2V 519Ah / 26kWh

	Dimensions
	Not provided
	Not provided
	Not provided
	Not provided

	Net weight
	87kg
	129kg
	132.2kg
	174kg

	Transfer time
	Not provided
	Not provided
	Not provided
	Not provided

	Efficiency
	Not provided
	Not provided
	Not provided
	Not provided

	Model configuration — Rated capacity
	10KWH
	15KWH
	18KWH
	26KWH

	Model configuration — Battery configuration
	51.2V 200Ah / 10kWh
	51.2V 300Ah / 15kWh
	51.2V 346Ah / 18kWh
	51.2V 519Ah / 26kWh

	Model configuration — Net weight
	87kg
	129kg
	132.2kg
	174kg

	Battery — Battery configuration
	16S1P
	16S1P
	16S1P
	16S1P

	Battery — Battery energy
	10kWh (catalog rating)
	15kWh (catalog rating)
	18kWh (catalog rating)
	26kWh (catalog rating)

	Communication & Monitoring — Communication interface
	RS485 / CAN
	RS485 / CAN
	RS485 / CAN
	RS485 / CAN

	Communication & Monitoring — Battery management
	BMS
	BMS
	BMS
	BMS

	Communication & Monitoring — Display
	LCD (optional)
	LCD (optional)
	LCD (optional)
	LCD (optional)

	Packaging — Package dimensions
	725×520×310mm
	740×570×420mm
	740×570×420mm
	1050×665×215mm

	Packaging — Wooden crate dimensions
	765×550×445mm
	775×600×555mm
	775×600×555mm
	1200×700×320mm

	Packaging — Gross weight
	105.15kg
	146kg
	149.2kg
	194kg

	Accessories — Accessories
	Positive/negative cables: 1200mm × 1 each; RJ45 (RS485): 1500mm × 1; User manual
	Positive/negative cables: 1200mm × 1 each; RJ45 (RS485): 1500mm × 1; User manual
	Positive/negative cables: 1200mm × 1 each; RJ45 (RS485): 1500mm × 1; User manual
	Positive/negative cables: 1200mm × 1 each; RJ45 (RS485): 1500mm × 1; User manual
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