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UPS UNINTERRUPTIBLE POWER SUPPLY
APS Series Portable Power Stations
Exact model: APS-PORTABLE-POWER-STATION
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	APS-PORTABLE-POWER-STATION · Primary



PRODUCT OVERVIEW
APS Series Portable Power Stations with 2 source-reviewed models for Mobile service teams, emergency backup, field communications and lighting. Model configuration and destination-market requirements are confirmed during RFQ review.
	Product line
	UPS Uninterruptible Power Supply

	Series / family
	Standalone model

	Exact model
	APS-PORTABLE-POWER-STATION

	Applications
	Mobile service teams, emergency backup, field communications and lighting


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Topology
	Power Range
	Phase

	APS-PORTABLE-POWER-STATION
	APS Series Portable Power Stations
	Portable LiFePO4 power station
	APS-500W to APS-1000W
	AC, solar and vehicle charging input / AC and DC output


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Topology
	Portable LiFePO4 power station

	Power Range
	APS-500W to APS-1000W

	Phase
	AC, solar and vehicle charging input / AC and DC output

	Form Factor
	Portable

	Waveform
	Sine wave

	Power Factor
	Model-specific; confirm on quotation

	Battery Types
	Source-defined lithium or LiFePO4 configuration

	SKU
	APS-PORTABLE-POWER-STATION

	Available Configurations
	APS-500W; APS-1000W

	Exact Configuration
	Confirm one listed configuration during RFQ review

	Destination Requirements
	To be confirmed


ENGINEERING TABLES
APS-PORTABLE-POWER-STATION · Complete Model Specifications — APS-500W | APS-1000W
	Parameter
	APS-500W
	APS-1000W

	Rated capacity
	APS-500W
	APS-1000W

	Battery configuration
	307WH 12.8V/24AH
	615WH 12.8V/48AH

	Dimensions
	366x169x175
	366x169x175

	Net weight
	6.6kg
	9.7kg

	Transfer time
	Not provided
	Not provided

	Efficiency
	Not provided
	Not provided

	Input — AC input
	INV mode INV 70~145VAC OR 140 ~260VAC
	INV mode INV 70~145VAC OR 140 ~260VAC

	Input — AC charging
	14.4V/8A
	14.4V/8A

	Input — Solar charging
	10A (max)
	10A (max)

	AC — Output voltage
	220Vac
	220Vac

	AC — Output frequency
	50Hz or 60Hz
	50Hz or 60Hz

	AC — Output waveform
	sine wave
	sine wave

	AC — Max output power
	500W
	1000W

	Technical Data — DC port
	12V/10A(max)
	12V/10A(max)

	Technical Data — Net weight
	6.6kg
	9.7kg

	DC — USB
	2*5V/2.4A USB-A ports + 1*QC2.0 fast chargingUSB-A port_ 2 5V/2.4AUSB-A +1 QC2.0 USB-A
	2*5V/2.4A USB-A ports + 1*QC2.0 fast chargingUSB-A port_ 2 5V/2.4AUSB-A +1 QC2.0 USB-A

	Battery Specification — Battery type
	LiFePO4
	LiFePO4

	Battery Specification — Battery Numbers
	16
	32

	Battery Specification — Battery capacity
	307WH 12.8V/24AH
	615WH 12.8V/48AH

	Physical Parameters — Size /(mm)
	366x169x175
	366x169x175
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