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UPS UNINTERRUPTIBLE POWER SUPPLY
AR Series Line-Interactive UPS
Exact model: AR-LINE-INTERACTIVE-UPS
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	AR-LINE-INTERACTIVE-UPS · Primary



PRODUCT OVERVIEW
AR Series Line-Interactive UPS with 3 source-reviewed models for Office PCs, POS terminals, CCTV recorders and small network equipment. Model configuration and destination-market requirements are confirmed during RFQ review.
	Product line
	UPS Uninterruptible Power Supply

	Series / family
	Standalone model

	Exact model
	AR-LINE-INTERACTIVE-UPS

	Applications
	Office PCs, POS terminals, CCTV recorders and small network equipment


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Topology
	Power Range
	Phase

	AR-LINE-INTERACTIVE-UPS
	AR Series Line-Interactive UPS
	Line-interactive UPS with AVR
	650VA/360W to 1000VA/600W
	Single phase input / Single phase output


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Topology
	Line-interactive UPS with AVR

	Power Range
	650VA/360W to 1000VA/600W

	Phase
	Single phase input / Single phase output

	Form Factor
	Tower

	Waveform
	Simulated sine wave

	Power Factor
	Model-specific; confirm on quotation

	Battery Types
	Model-dependent

	SKU
	AR-LINE-INTERACTIVE-UPS

	Available Configurations
	AR650; AR850; AR1000

	Exact Configuration
	Confirm one listed configuration during RFQ review

	Destination Requirements
	To be confirmed


ENGINEERING TABLES
AR-LINE-INTERACTIVE-UPS · Complete Model Specifications — AR650 | AR850 | AR1000
	Parameter
	AR650
	AR850
	AR1000

	Rated capacity
	650VA/360W
	850VA/480W
	1000VA/600W

	Battery configuration
	12V/7Ah × 1
	12V/9Ah × 1
	12V/9Ah × 1

	Dimensions
	115×115×40mm
	115×115×40mm
	115×115×40mm

	Net weight
	5.8kg
	6kg
	6kg

	Transfer time
	4-6ms
	4-6ms
	4-6ms

	Efficiency
	Not provided
	Not provided
	Not provided

	Model configuration — Rated capacity
	650VA/360W
	850VA/480W
	1000VA/600W

	Model configuration — Battery configuration
	12V/7Ah × 1
	12V/9Ah × 1
	12V/9Ah × 1

	Model configuration — Product dimensions
	115×115×40mm
	115×115×40mm
	115×115×40mm

	Model configuration — Net weight
	5.8kg
	6kg
	6kg

	Model configuration — Transfer time
	4-6ms
	4-6ms
	4-6ms

	Input — Input voltage
	110/120VAC or 220/230/240VAC
	110/120VAC or 220/230/240VAC
	110/120VAC or 220/230/240VAC

	Input — Input voltage range
	81–145VAC or 145–275VAC
	81–145VAC or 145–275VAC
	81–145VAC or 145–275VAC

	Input — Input frequency
	50/60Hz (auto sensing)
	50/60Hz (auto sensing)
	50/60Hz (auto sensing)

	Output — Output voltage
	110/120VAC or 220/230/240VAC
	110/120VAC or 220/230/240VAC
	110/120VAC or 220/230/240VAC

	Output — Voltage regulation
	±10%
	±10%
	±10%

	Output — Battery-mode frequency
	50/60Hz ±1Hz
	50/60Hz ±1Hz
	50/60Hz ±1Hz

	Output — Output waveform
	Simulated sine wave
	Simulated sine wave
	Simulated sine wave

	Charging — Charging time
	8h to 90% capacity
	8h to 90% capacity
	8h to 90% capacity

	Protection — Protection function
	Discharge, short circuit and overload
	Discharge, short circuit and overload
	Discharge, short circuit and overload

	Display & Alarms — Display
	LCD
	LCD
	LCD

	Display & Alarms — Battery mode alarm
	Every 4 seconds
	Every 4 seconds
	Every 4 seconds

	Display & Alarms — Low battery alarm
	Every second
	Every second
	Every second

	Display & Alarms — Overload alarm
	Every second
	Every second
	Every second

	Display & Alarms — Fault alarm
	Continuous
	Continuous
	Continuous

	Communication & Monitoring — Communication interface
	RJ45 / USB 5V (2A)
	RJ45 / USB 5V (2A)
	RJ45 / USB 5V (2A)

	Environment — Operating temperature
	0–40°C
	0–40°C
	0–40°C

	Environment — Relative humidity
	0–90% RH (non-condensing)
	0–90% RH (non-condensing)
	0–90% RH (non-condensing)

	Environment — Noise level
	<40dB
	<40dB
	<40dB
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