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UPS UNINTERRUPTIBLE POWER SUPPLY
DC Series Mini DC UPS
Exact model: DC-SERIES-MINI-UPS
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PRODUCT OVERVIEW
DC Series Mini DC UPS with 8 source-reviewed models for Routers, ONT devices, CCTV cameras and IoT equipment. Model configuration and destination-market requirements are confirmed during RFQ review.
	Product line
	UPS Uninterruptible Power Supply

	Series / family
	Standalone model

	Exact model
	DC-SERIES-MINI-UPS

	Applications
	Routers, ONT devices, CCTV cameras and IoT equipment


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Topology
	Power Range
	Phase

	DC-SERIES-MINI-UPS
	DC Series Mini DC UPS
	Compact DC backup UPS
	18W–36W
	85–265VAC, 50–60Hz input / DC / USB / PoE options output


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Topology
	Compact DC backup UPS

	Power Range
	18W–36W

	Phase
	85–265VAC, 50–60Hz input / DC / USB / PoE options output

	Form Factor
	Compact desktop

	Waveform
	Regulated DC

	Power Factor
	Model-specific; confirm on quotation

	Battery Types
	Lithium-ion / LiFePO4

	SKU
	DC-SERIES-MINI-UPS

	Available Configurations
	DC1018C; DC1018CP; DC1018; DC1018P; DC1036C; DC1036CP; DC1036; DC1036P

	Exact Configuration
	Confirm one listed configuration during RFQ review

	Destination Requirements
	To be confirmed


ENGINEERING TABLES
DC-SERIES-MINI-UPS · Complete Model Specifications — DC1018C | DC1018CP | DC1018 | DC1018P
	Parameter
	DC1018C
	DC1018CP
	DC1018
	DC1018P

	Rated capacity
	18W
	18W
	18W
	18W

	Battery configuration
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell

	Dimensions
	160×105×33mm
	160×105×33mm
	160×105×33mm
	160×105×33mm

	Net weight
	0.38kg
	0.4kg
	0.39kg
	0.39kg

	Transfer time
	Not provided
	Not provided
	Not provided
	Not provided

	Efficiency
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%

	Model configuration — Rated capacity
	18W
	18W
	18W
	18W

	Model configuration — Battery configuration
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell

	Model configuration — Product dimensions
	160×105×33mm
	160×105×33mm
	160×105×33mm
	160×105×33mm

	Model configuration — Net weight
	0.38kg
	0.4kg
	0.39kg
	0.39kg

	Model configuration — Efficiency
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%

	Input — Input voltage
	85–265VAC
	85–265VAC
	85–265VAC
	85–265VAC

	Input — Input frequency
	50–60Hz
	50–60Hz
	50–60Hz
	50–60Hz

	Battery — Battery chemistry
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4

	Battery — Battery cell size
	18650
	18650
	18650
	18650

	Battery — Cell capacity
	2000–2600mAh
	2000–2600mAh
	2000–2600mAh
	2000–2600mAh

	Battery — Battery quantity
	4
	4
	4
	4

	Protection — Protection function
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit

	Environment — Operating temperature
	0–40°C
	0–40°C
	0–40°C
	0–40°C

	Environment — Storage temperature
	-10–70°C
	-10–70°C
	-10–70°C
	-10–70°C

	Environment — Relative humidity
	10–90% RH
	10–90% RH
	10–90% RH
	10–90% RH

	Environment — Altitude
	<3000m
	<3000m
	<3000m
	<3000m

	Environment — Noise level
	<30dB
	<30dB
	<30dB
	<30dB

	Housing — Housing material
	ABS
	ABS
	ABS
	ABS

	Housing — Housing color
	Black / White
	Black / White
	Black / White
	Black / White

	Output — USB output
	5V/2A
	5V/2A
	5V/2A
	5V/2A

	Output — DC output
	9V(12V)/1A
	9V(12V)/1A
	5V/2A; 9V/1A; 12V/1A
	5V/2A; 9V/1A; 12V/1A

	Physical — Package dimensions
	180×160×37mm
	180×160×37mm
	180×160×37mm
	180×160×37mm

	Physical — Gross weight
	0.51kg
	0.53kg
	0.5kg
	0.52kg

	Output — PoE output
	Not provided
	15V/0.6A; 24V/0.6A
	Not provided
	15V/0.6A; 24V/0.6A


DC-SERIES-MINI-UPS · Complete Model Specifications — DC1036C | DC1036CP | DC1036 | DC1036P
	Parameter
	DC1036C
	DC1036CP
	DC1036
	DC1036P

	Rated capacity
	36W
	36W
	36W
	36W

	Battery configuration
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell

	Dimensions
	160×105×33mm
	160×105×33mm
	160×105×33mm
	160×105×33mm

	Net weight
	0.39kg
	0.41kg
	0.4kg
	0.42kg

	Transfer time
	Not provided
	Not provided
	Not provided
	Not provided

	Efficiency
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%

	Model configuration — Rated capacity
	36W
	36W
	36W
	36W

	Model configuration — Battery configuration
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell

	Model configuration — Product dimensions
	160×105×33mm
	160×105×33mm
	160×105×33mm
	160×105×33mm

	Model configuration — Net weight
	0.39kg
	0.41kg
	0.4kg
	0.42kg

	Model configuration — Efficiency
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%

	Input — Input voltage
	85–265VAC
	85–265VAC
	85–265VAC
	85–265VAC

	Input — Input frequency
	50–60Hz
	50–60Hz
	50–60Hz
	50–60Hz

	Battery — Battery chemistry
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4

	Battery — Battery cell size
	18650
	18650
	18650
	18650

	Battery — Cell capacity
	2000–2600mAh
	2000–2600mAh
	2000–2600mAh
	2000–2600mAh

	Battery — Battery quantity
	4
	4
	4
	4

	Protection — Protection function
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit

	Environment — Operating temperature
	0–40°C
	0–40°C
	0–40°C
	0–40°C

	Environment — Storage temperature
	-10–70°C
	-10–70°C
	-10–70°C
	-10–70°C

	Environment — Relative humidity
	10–90% RH
	10–90% RH
	10–90% RH
	10–90% RH

	Environment — Altitude
	<3000m
	<3000m
	<3000m
	<3000m

	Environment — Noise level
	<30dB
	<30dB
	<30dB
	<30dB

	Housing — Housing material
	ABS
	ABS
	ABS
	ABS

	Housing — Housing color
	Black / White
	Black / White
	Black / White
	Black / White

	Output — USB output
	5V/2A
	5V/2A
	5V/2A
	5V/2A

	Output — DC output
	9V/12V (3A)
	9V/12V (3A)
	5V/2A; 9V/2A; 12V/2A
	5V/2A; 9V/2A; 12V/2A

	Physical — Package dimensions
	180×160×37mm
	180×160×37mm
	180×160×37mm
	180×160×37mm

	Physical — Gross weight
	0.52kg
	0.55kg
	0.51kg
	0.56kg

	Output — PoE output
	Not provided
	15V/1A; 24V/1A
	Not provided
	15V/1A; 24V/1A
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