
	[image: ]
	PRODUCT SPECIFICATION
Standalone model


[image: ]
UPS UNINTERRUPTIBLE POWER SUPPLY
DCP Series Multi-Output DC UPS
Exact model: DCP-SERIES-DC-UPS
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PRODUCT OVERVIEW
DCP Series Multi-Output DC UPS with 10 source-reviewed models for Routers, CCTV cameras, access control and PoE edge devices. Model configuration and destination-market requirements are confirmed during RFQ review.
	Product line
	UPS Uninterruptible Power Supply

	Series / family
	Standalone model

	Exact model
	DCP-SERIES-DC-UPS

	Applications
	Routers, CCTV cameras, access control and PoE edge devices


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Topology
	Power Range
	Phase

	DCP-SERIES-DC-UPS
	DCP Series Multi-Output DC UPS
	Multi-output DC backup UPS
	18W DC UPS to 120W DC UPS
	AC or DC adapter input / DC, USB and PoE options output


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Topology
	Multi-output DC backup UPS

	Power Range
	18W DC UPS to 120W DC UPS

	Phase
	AC or DC adapter input / DC, USB and PoE options output

	Form Factor
	Compact desktop

	Waveform
	Regulated DC

	Power Factor
	Model-specific; confirm on quotation

	Battery Types
	Lithium-ion / LiFePO4

	SKU
	DCP-SERIES-DC-UPS

	Available Configurations
	DCP-018W; DCP-18W; DCP-6018W; DCP-36W; DCP-6036W; DCP-045W; DCP-060W; DCP-60W; DCP-100W; DCP-120W

	Exact Configuration
	Confirm one listed configuration during RFQ review

	Destination Requirements
	To be confirmed


ENGINEERING TABLES
DCP-SERIES-DC-UPS · Complete Model Specifications — DCP-018W | DCP-18W | DCP-6018W | DCP-36W
	Parameter
	DCP-018W
	DCP-18W
	DCP-6018W
	DCP-36W

	Rated capacity
	18W DC UPS
	18W DC UPS
	18W DC UPS
	36W DC UPS

	Battery configuration
	4 cells; 18650
	4 cells; 18650
	4/8 cells; 18650/21700/32700
	4 cells; 18650

	Dimensions
	128mm*77mm*27mm
	180mm*106*40mm
	214mm*158.5mm*86mm
	180*106*40mm

	Net weight
	0.26kg
	0.43kg
	1.68kg (max)
	0.43kg

	Transfer time
	Not provided
	Not provided
	Not provided
	Not provided

	Efficiency
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%

	Model configuration — Rated capacity
	18W DC UPS
	18W DC UPS
	18W DC UPS
	36W DC UPS

	Model configuration — Battery configuration
	4 cells; 18650
	4 cells; 18650
	4/8 cells; 18650/21700/32700
	4 cells; 18650

	Model configuration — Product dimensions
	128mm*77mm*27mm
	180mm*106*40mm
	214mm*158.5mm*86mm
	180*106*40mm

	Model configuration — Net weight
	0.26kg
	0.43kg
	1.68kg (max)
	0.43kg

	Model configuration — Efficiency
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%

	Technical Data — Maximum output power
	18W
	18W
	18W
	36W

	Technical Data — Input
	DC 9V/2A max.
	AC 100–240V, 50–60Hz
	AC 100–240V, 50–60Hz
	AC 100–240V, 50–60Hz

	Technical Data — Output ports
	USB 5V/2A; DC 9V/1A; DC 12V/1A
	USB 5V/2A; DC 5V/2A; DC 9V/1A; DC 12V/1A; PoE 15V/0.6A; PoE 24V/0.6A
	USB 5V/2A; DC 5V/2A; DC 9V/1A; DC 12V/1A; PoE 15V/0.6A; PoE 24V/0.6A
	USB 5V/2A; DC 5V/2A; DC 9V/1A; DC 12V/1A; PoE 15V/1A; PoE 24V/1A

	Technical Data — Battery cell size
	18650
	18650
	18650/21700/32700
	18650

	Technical Data — Cell capacity
	2000-2600mah
	2000-2600mah
	2000-6000mah
	2000-2600mah

	Technical Data — Battery quantity
	4
	4
	4/8
	4

	Technical Data — Efficiency
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%

	Technical Data — Battery chemistry
	Lithium-ion or LiFePO4
	Lithium-ion or LiFePO4
	Lithium-ion or LiFePO4
	Lithium-ion or LiFePO4

	Technical Data — Housing
	ABS, black or white
	ABS, black or white
	ABS, black or white
	ABS, black or white

	Technical Data — Protection
	Over-charge, over-discharge, over-current, overload, over-temperature and short-circuit protection
	Over-charge, over-discharge, over-current, overload, over-temperature and short-circuit protection
	Over-charge, over-discharge, over-current, overload, over-temperature and short-circuit protection
	Over-charge, over-discharge, over-current, overload, over-temperature and short-circuit protection

	Technical Data — Operating temperature
	0–40°C
	0–40°C
	0–40°C
	0–40°C

	Technical Data — Storage temperature
	-10–70°C
	-10–70°C
	-10–70°C
	-10–70°C

	Technical Data — Humidity
	10–90% RH
	10–90% RH
	10–90% RH
	10–90% RH

	Technical Data — Altitude
	<3000 m
	<3000 m
	<3000 m
	<3000 m

	Technical Data — Noise
	<30 dB
	<30 dB
	<30 dB
	<30 dB

	Technical Data — Product dimensions
	128mm*77mm*27mm
	180mm*106*40mm
	214mm*158.5mm*86mm
	180*106*40mm

	Technical Data — Package dimensions
	178mm*85mm*33mm(Without adaptor)
	190mm*160mm*50mm
	230mm*230mm*95mm
	190mm*160mm*50mm

	Technical Data — Net weight
	0.26kg
	0.43kg
	1.68kg (max)
	0.43kg

	Technical Data — Gross weight
	0.32kg
	0.56kg
	2.43kg (max)
	0.56kg


DCP-SERIES-DC-UPS · Complete Model Specifications — DCP-6036W | DCP-045W | DCP-060W | DCP-60W
	Parameter
	DCP-6036W
	DCP-045W
	DCP-060W
	DCP-60W

	Rated capacity
	36W DC UPS
	45W DC UPS
	60W DC UPS
	60W DC UPS

	Battery configuration
	4/8 cells; 18650/21700/32700
	4/8 cells; 18650
	4/8 cells; 18650
	4/8 cells; 18650/21700/32700

	Dimensions
	214mm*158.5mm*86mm
	180mm*130mm*64mm
	180mm*130mm*64mm
	214mm*158.5mm*86mm

	Net weight
	1.69kg (max)
	0.83kg (max)
	0.85kg (max)
	1.85kg (max)

	Transfer time
	Not provided
	Not provided
	Not provided
	Not provided

	Efficiency
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%

	Model configuration — Rated capacity
	36W DC UPS
	45W DC UPS
	60W DC UPS
	60W DC UPS

	Model configuration — Battery configuration
	4/8 cells; 18650/21700/32700
	4/8 cells; 18650
	4/8 cells; 18650
	4/8 cells; 18650/21700/32700

	Model configuration — Product dimensions
	214mm*158.5mm*86mm
	180mm*130mm*64mm
	180mm*130mm*64mm
	214mm*158.5mm*86mm

	Model configuration — Net weight
	1.69kg (max)
	0.83kg (max)
	0.85kg (max)
	1.85kg (max)

	Model configuration — Efficiency
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%

	Technical Data — Maximum output power
	36W
	45W
	60W
	60W

	Technical Data — Input
	AC 100–240V, 50–60Hz
	AC 100–240V, 50–60Hz
	AC 100–240V, 50–60Hz
	AC 100–240V, 50–60Hz

	Technical Data — Output ports
	USB 5V/2A; DC 5V/2A; DC 9V/1A; DC 12V/1A; PoE 15V/1A; PoE 24V/1A; PoE 48V/0.6A
	USB 5V/2.4A; DC 5V/2.4A; DC 9V(12V)/2A; DC 12V/3.5A; PoE 15V/1.5A; PoE 24V/1A; PoE 48V/0.6A
	USB 5V/2.4A; DC 5V/2.4A; DC 9V(12V)/2A; DC 12V/5A; PoE 15V/1.5A; PoE 24V/1A; PoE 48V/0.6A
	USB 5V/2.4A; DC 5V/2.4A; DC 9V(12V)/2A; DC 12V/5A; DC 19V/3A; PoE 15V/1.5A; PoE 24V/1A; PoE 48V/0.6A (optional)

	Technical Data — Battery cell size
	18650/21700/32700
	18650
	18650
	18650/21700/32700

	Technical Data — Cell capacity
	2000-6000mah
	2000-2600mah
	2000-2600mah
	2000-6000mah

	Technical Data — Battery quantity
	4/8
	4/8
	4/8
	4/8

	Technical Data — Efficiency
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%

	Technical Data — Battery chemistry
	Lithium-ion or LiFePO4
	Lithium-ion or LiFePO4
	Lithium-ion or LiFePO4
	Lithium-ion or LiFePO4

	Technical Data — Housing
	ABS, black or white
	ABS, black or white
	ABS, black or white
	ABS, black or white

	Technical Data — Protection
	Over-charge, over-discharge, over-current, overload, over-temperature and short-circuit protection
	Over-charge, over-discharge, over-current, overload, over-temperature and short-circuit protection
	Over-charge, over-discharge, over-current, overload, over-temperature and short-circuit protection
	Over-charge, over-discharge, over-current, overload, over-temperature and short-circuit protection

	Technical Data — Operating temperature
	0–40°C
	0–40°C
	0–40°C
	0–40°C

	Technical Data — Storage temperature
	-10–70°C
	-10–70°C
	-10–70°C
	-10–70°C

	Technical Data — Humidity
	10–90% RH
	10–90% RH
	10–90% RH
	10–90% RH

	Technical Data — Altitude
	<3000 m
	<3000 m
	<3000 m
	<3000 m

	Technical Data — Noise
	<30 dB
	<30 dB
	<30 dB
	<45 dB

	Technical Data — Product dimensions
	214mm*158.5mm*86mm
	180mm*130mm*64mm
	180mm*130mm*64mm
	214mm*158.5mm*86mm

	Technical Data — Package dimensions
	230mm*230mm*95mm
	195mm*180mm*70mm
	195mm*180mm*70mm
	230mm*230mm*95mm

	Technical Data — Net weight
	1.69kg (max)
	0.83kg (max)
	0.85kg (max)
	1.85kg (max)

	Technical Data — Gross weight
	2.44kg (max)
	1.2kg (max)
	1.3kg (max)
	2.6kg (max)


DCP-SERIES-DC-UPS · Complete Model Specifications — DCP-100W | DCP-120W
	Parameter
	DCP-100W
	DCP-120W

	Rated capacity
	100W DC UPS
	120W DC UPS

	Battery configuration
	4/8 cells; 18650/21700/32700
	4/8 cells; 18650/21700/32700

	Dimensions
	214mm*158.5mm*86mm
	214mm*158.5mm*86mm

	Net weight
	1.88kg (max)
	1.9kg (max)

	Transfer time
	Not provided
	Not provided

	Efficiency
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%

	Model configuration — Rated capacity
	100W DC UPS
	120W DC UPS

	Model configuration — Battery configuration
	4/8 cells; 18650/21700/32700
	4/8 cells; 18650/21700/32700

	Model configuration — Product dimensions
	214mm*158.5mm*86mm
	214mm*158.5mm*86mm

	Model configuration — Net weight
	1.88kg (max)
	1.9kg (max)

	Model configuration — Efficiency
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%

	Technical Data — Maximum output power
	100W
	120W

	Technical Data — Input
	AC 100–240V, 50–60Hz
	AC 100–240V, 50–60Hz

	Technical Data — Output ports
	USB 5V/2.4A; DC 5V/2.4A; DC 9V(12V)/2A; DC 12V/8A; DC 19V/5A; PoE 15V/1.5A; PoE 24V/1A; PoE 48V/0.6A (optional)
	USB 5V/2.4A; DC 5V/2.4A; DC 9V(12V)/2A; DC 12V/10A; DC 19V/6A; PoE 15V/1.5A; PoE 24V/1A; PoE 48V/0.6A (optional)

	Technical Data — Battery cell size
	18650/21700/32700
	18650/21700/32700

	Technical Data — Cell capacity
	2000-6000mah
	2000-6000mah

	Technical Data — Battery quantity
	4/8
	4/8

	Technical Data — Efficiency
	AC mode >85%; battery mode >90%
	AC mode >85%; battery mode >90%

	Technical Data — Battery chemistry
	Lithium-ion or LiFePO4
	Lithium-ion or LiFePO4

	Technical Data — Housing
	ABS, black or white
	ABS, black or white

	Technical Data — Protection
	Over-charge, over-discharge, over-current, overload, over-temperature and short-circuit protection
	Over-charge, over-discharge, over-current, overload, over-temperature and short-circuit protection

	Technical Data — Operating temperature
	0–40°C
	0–40°C

	Technical Data — Storage temperature
	-10–70°C
	-10–70°C

	Technical Data — Humidity
	10–90% RH
	10–90% RH

	Technical Data — Altitude
	<3000 m
	<3000 m

	Technical Data — Noise
	<45 dB
	<45 dB

	Technical Data — Product dimensions
	214mm*158.5mm*86mm
	214mm*158.5mm*86mm

	Technical Data — Package dimensions
	230mm*230mm*95mm
	230mm*230mm*95mm

	Technical Data — Net weight
	1.88kg (max)
	1.9kg (max)

	Technical Data — Gross weight
	2.63kg (max)
	2.65kg (max)
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