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UPS UNINTERRUPTIBLE POWER SUPPLY
Line-Interactive UPS 650VA-2000VA Series
Exact model: NX-UP-ST-002
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PRODUCT OVERVIEW
Line-interactive UPS with AVR providing enhanced voltage regulation for environments with frequent power fluctuations. Six models from 650VA to 2000VA.
	Product line
	UPS Uninterruptible Power Supply

	Series / family
	Standalone model

	Exact model
	NX-UP-ST-002

	Applications
	Small offices, Home offices, POS terminals, Security systems, Printers and peripherals


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Topology
	Power Range
	Phase

	NX-UP-ST-002
	Line-Interactive UPS 650VA-2000VA Series
	Line-Interactive with AVR
	650VA-2000VA / 390W-1200W
	Single phase input / Single phase output


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Topology
	Line-Interactive with AVR

	Power Range
	650VA-2000VA / 390W-1200W

	Phase
	Single phase input / Single phase output

	Form Factor
	Tower

	Waveform
	Simulated sine wave

	Power Factor
	0.6

	Battery Types
	VRLA sealed lead-acid

	SKU
	NX-UP-ST-002

	Available Configurations
	AK650; AK850; AK1000; AK1200; AK1500; AK2000

	Exact Configuration
	Confirm one listed configuration during RFQ review

	Destination Requirements
	To be confirmed


ENGINEERING TABLES
NX-UP-ST-002 · Complete Model Specifications — AK650 | AK850 | AK1000 | AK1200
	Parameter
	AK650
	AK850
	AK1000
	AK1200

	Rated capacity
	650VA / 390W
	850VA / 510W
	1000VA / 600W
	1200VA / 720W

	Battery configuration
	Not provided
	Not provided
	Not provided
	Not provided

	Dimensions
	Not provided
	Not provided
	Not provided
	Not provided

	Net weight
	Not provided
	Not provided
	Not provided
	Not provided

	Transfer time
	6ms
	6ms
	6ms
	6ms

	Efficiency
	Not provided
	Not provided
	Not provided
	Not provided

	Model configuration — Rated capacity
	650VA / 390W
	850VA / 510W
	1000VA / 600W
	1200VA / 720W

	Model configuration — Transfer time
	6ms
	6ms
	6ms
	6ms

	Input — Input voltage
	110/120VAC or 220/230/240VAC
	110/120VAC or 220/230/240VAC
	110/120VAC or 220/230/240VAC
	110/120VAC or 220/230/240VAC

	Input — Input voltage range
	86–140VAC or 170–285VAC
	86–140VAC or 170–285VAC
	86–140VAC or 170–285VAC
	86–140VAC or 170–285VAC

	Input — Input frequency
	50/60Hz
	50/60Hz
	50/60Hz
	50/60Hz

	Input — Input power factor
	≥0.999
	≥0.999
	≥0.999
	≥0.999

	Input — Wiring
	L+N+PE
	L+N+PE
	L+N+PE
	L+N+PE

	Output — Output voltage
	110/120VAC or 220/230/240VAC
	110/120VAC or 220/230/240VAC
	110/120VAC or 220/230/240VAC
	110/120VAC or 220/230/240VAC

	Output — Voltage regulation
	±10%
	±10%
	±10%
	±10%

	Output — Output frequency
	50/60Hz ±1Hz
	50/60Hz ±1Hz
	50/60Hz ±1Hz
	50/60Hz ±1Hz

	Output — Output power factor
	0.6
	0.6
	0.6
	0.6

	Charging — Charging current
	1A
	1A
	1A
	1A

	Communication & Monitoring — Communication interface
	RS232 / USB / RJ11 / RJ45
	RS232 / USB / RJ11 / RJ45
	RS232 / USB / RJ11 / RJ45
	RS232 / USB / RJ11 / RJ45

	Communication & Monitoring — Display
	LCD
	LCD
	LCD
	LCD

	Environment — Operating temperature
	-25–55°C
	-25–55°C
	-25–55°C
	-25–55°C

	Environment — Relative humidity
	20–95% RH (non-condensing)
	20–95% RH (non-condensing)
	20–95% RH (non-condensing)
	20–95% RH (non-condensing)

	Environment — Noise level
	<40dBA @1m
	<40dBA @1m
	<40dBA @1m
	<40dBA @1m

	Packaging — Package dimensions
	390×313×440mm
	390×313×440mm
	390×313×440mm
	450×436×250mm

	Packaging — Package weight
	20.8kg
	22.8kg
	23.2kg
	23.8kg

	Packaging — Units per carton
	4
	4
	4
	2


NX-UP-ST-002 · Complete Model Specifications — AK1500 | AK2000
	Parameter
	AK1500
	AK2000

	Rated capacity
	1500VA / 900W
	2000VA / 1200W

	Battery configuration
	Not provided
	Not provided

	Dimensions
	Not provided
	Not provided

	Net weight
	Not provided
	Not provided

	Transfer time
	6ms
	6ms

	Efficiency
	Not provided
	Not provided

	Model configuration — Rated capacity
	1500VA / 900W
	2000VA / 1200W

	Model configuration — Transfer time
	6ms
	6ms

	Input — Input voltage
	110/120VAC or 220/230/240VAC
	110/120VAC or 220/230/240VAC

	Input — Input voltage range
	86–140VAC or 170–285VAC
	86–140VAC or 170–285VAC

	Input — Input frequency
	50/60Hz
	50/60Hz

	Input — Input power factor
	≥0.999
	≥0.999

	Input — Wiring
	L+N+PE
	L+N+PE

	Output — Output voltage
	110/120VAC or 220/230/240VAC
	110/120VAC or 220/230/240VAC

	Output — Voltage regulation
	±10%
	±10%

	Output — Output frequency
	50/60Hz ±1Hz
	50/60Hz ±1Hz

	Output — Output power factor
	0.6
	0.6

	Charging — Charging current
	1A
	1A

	Communication & Monitoring — Communication interface
	RS232 / USB / RJ11 / RJ45
	RS232 / USB / RJ11 / RJ45

	Communication & Monitoring — Display
	LCD
	LCD

	Environment — Operating temperature
	-25–55°C
	-25–55°C

	Environment — Relative humidity
	20–95% RH (non-condensing)
	20–95% RH (non-condensing)

	Environment — Noise level
	<40dBA @1m
	<40dBA @1m

	Packaging — Package dimensions
	450×436×250mm
	450×436×250mm

	Packaging — Package weight
	25.2kg
	34kg

	Packaging — Units per carton
	2
	2
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