
	[image: ]
	PRODUCT SPECIFICATION
AL-PH Integrated Home Energy Storage
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UPS UNINTERRUPTIBLE POWER SUPPLY
AL-PH Integrated Home Energy Storage
Exact model: AL-PH-INTEGRATED-ESS
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	AL-PH-INTEGRATED-ESS · Primary



PRODUCT OVERVIEW
AL-PH Integrated Home Energy Storage with 2 source-reviewed models for Residential backup, solar self-consumption and off-grid homes. Model configuration and destination-market requirements are confirmed during RFQ review.
	Product line
	UPS Uninterruptible Power Supply

	Series / family
	Standalone model

	Exact model
	AL-PH-INTEGRATED-ESS

	Applications
	Residential backup, solar self-consumption and off-grid homes


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Topology
	Power Range
	Phase

	AL-PH-INTEGRATED-ESS
	AL-PH Integrated Home Energy Storage
	Integrated inverter and LiFePO4 storage
	3.6KW / 7.68KWH to 6KW / 16KWH
	AC and PV input / Single phase AC output


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Topology
	Integrated inverter and LiFePO4 storage

	Power Range
	3.6KW / 7.68KWH to 6KW / 16KWH

	Phase
	AC and PV input / Single phase AC output

	Form Factor
	Floor standing

	Waveform
	Pure sine wave

	Power Factor
	Model-specific; confirm on quotation

	Battery Types
	Source-defined lithium or LiFePO4 configuration

	SKU
	AL-PH-INTEGRATED-ESS

	Available Configurations
	AL-PH3.6KW-7.68KWH; AL-PH6KW-16KWH

	Exact Configuration
	Confirm one listed configuration during RFQ review

	Destination Requirements
	To be confirmed


ENGINEERING TABLES
AL-PH-INTEGRATED-ESS · Complete Model Specifications — AL-PH3.6KW-7.68KWH | AL-PH6KW-16KWH
	Parameter
	AL-PH3.6KW-7.68KWH
	AL-PH6KW-16KWH

	Rated capacity
	3.6KW / 7.68KWH
	6KW / 16KWH

	Battery configuration
	25.6V 300Ah / 7.68kWh
	51.2V 314Ah / 16kWh

	Dimensions
	740×400×240mm
	1040×460×240mm

	Net weight
	Not provided
	Not provided

	Transfer time
	Not provided
	Not provided

	Efficiency
	Not provided
	Not provided

	Model configuration — Rated capacity
	3.6KW / 7.68KWH
	6KW / 16KWH

	Model configuration — Battery configuration
	25.6V 300Ah / 7.68kWh
	51.2V 314Ah / 16kWh

	Model configuration — Product dimensions
	740×400×240mm
	1040×460×240mm

	Input — PV input power
	5000W
	9000W

	Input — PV charging voltage
	40–450V
	60–450V

	Input — Optimum PV voltage
	300–400V
	300–400V

	Input — Charging mode
	MPPT
	MPPT

	Output — Output voltage
	220–240VAC
	220–240VAC

	Output — Output frequency
	50/60Hz
	50/60Hz

	Battery — Battery energy
	7.68kWh
	16kWh

	Battery — Cycle life
	≥6000 cycles (supplier rating; conditions to be confirmed)
	≥6000 cycles (supplier rating; conditions to be confirmed)

	Packaging — Package dimensions
	750×410×250mm
	1050×470×250mm

	Packaging — Wooden crate dimensions
	760×420×260mm
	1060×480×260mm

	Packaging — Total weight
	67.5kg
	124kg

	Accessories — Accessories
	Charging cable × 1; User manual × 1
	Charging cable × 1; User manual × 1



	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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