
	[image: ]
	PRODUCT SPECIFICATION
AL-Vertical Home Energy Storage


[image: ]
UPS UNINTERRUPTIBLE POWER SUPPLY
AL-Vertical Home Energy Storage
Exact model: AL-VERTICAL-ESS
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PRODUCT OVERVIEW
AL-Vertical Home Energy Storage with 2 source-reviewed models for Residential solar storage and compact floor-standing backup systems. Model configuration and destination-market requirements are confirmed during RFQ review.
	Product line
	UPS Uninterruptible Power Supply

	Series / family
	Standalone model

	Exact model
	AL-VERTICAL-ESS

	Applications
	Residential solar storage and compact floor-standing backup systems


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Topology
	Power Range
	Phase

	AL-VERTICAL-ESS
	AL-Vertical Home Energy Storage
	Vertical integrated energy storage system
	5.5KW / 5.12KWH to 5.5KW / 10KWH
	AC and PV input / Single phase AC output


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Topology
	Vertical integrated energy storage system

	Power Range
	5.5KW / 5.12KWH to 5.5KW / 10KWH

	Phase
	AC and PV input / Single phase AC output

	Form Factor
	Floor standing

	Waveform
	Pure sine wave

	Power Factor
	Model-specific; confirm on quotation

	Battery Types
	Source-defined lithium or LiFePO4 configuration

	SKU
	AL-VERTICAL-ESS

	Available Configurations
	AL-VERTICAL-5KW.H; AL-VERTICAL-10KW.H

	Exact Configuration
	Confirm one listed configuration during RFQ review

	Destination Requirements
	To be confirmed


ENGINEERING TABLES
AL-VERTICAL-ESS · Complete Model Specifications — AL-VERTICAL-5KW.H | AL-VERTICAL-10KW.H
	Parameter
	AL-VERTICAL-5KW.H
	AL-VERTICAL-10KW.H

	Rated capacity
	5.5KW / 5.12KWH
	5.5KW / 10KWH

	Battery configuration
	5.12kWh × 1
	5.12kWh × 2

	Dimensions
	Not provided
	Not provided

	Net weight
	Not provided
	Not provided

	Transfer time
	Not provided
	Not provided

	Efficiency
	Not provided
	Not provided

	Model configuration — Rated capacity
	5.5KW / 5.12KWH
	5.5KW / 10KWH

	Model configuration — Battery configuration
	5.12kWh × 1
	5.12kWh × 2

	Input — DC input voltage
	120–500V
	120–500V

	Input — DC input power
	5500W
	5500W

	Output — Output voltage
	210–230VAC
	210–230VAC

	Output — Output frequency
	50/60Hz
	50/60Hz

	Output — Maximum power
	5500W
	5500W

	Battery — Battery energy
	5.12kWh
	5.12kWh × 2

	Battery — Battery configuration
	3.2V 100Ah; 16S1P per module
	3.2V 100Ah; 16S1P per module

	Packaging — Battery package dimensions
	670×500×285mm × 1
	670×500×285mm × 2

	Packaging — Wooden crate dimensions
	680×510×300mm × 1
	680×510×300mm × 2

	Packaging — Inverter package dimensions
	670×500×285mm
	670×500×285mm

	Packaging — Gross weight
	17.3kg + 66.05kg
	17.3kg + 66.05kg + 66.65kg
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