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UPS UNINTERRUPTIBLE POWER SUPPLY
DCF Series Mini DC UPS
Exact model: DCF-SERIES-MINI-UPS
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PRODUCT OVERVIEW
DCF Series Mini DC UPS with 8 source-reviewed models for Network edge devices, CCTV cameras and communications equipment. Model configuration and destination-market requirements are confirmed during RFQ review.
	Product line
	UPS Uninterruptible Power Supply

	Series / family
	Standalone model

	Exact model
	DCF-SERIES-MINI-UPS

	Applications
	Network edge devices, CCTV cameras and communications equipment


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Topology
	Power Range
	Phase

	DCF-SERIES-MINI-UPS
	DCF Series Mini DC UPS
	Display-equipped DC backup UPS
	18W–36W
	85–265VAC, 50–60Hz input / DC / USB / PoE options output


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Topology
	Display-equipped DC backup UPS

	Power Range
	18W–36W

	Phase
	85–265VAC, 50–60Hz input / DC / USB / PoE options output

	Form Factor
	Compact desktop

	Waveform
	Regulated DC

	Power Factor
	Model-specific; confirm on quotation

	Battery Types
	Lithium-ion / LiFePO4

	SKU
	DCF-SERIES-MINI-UPS

	Available Configurations
	DCF-1018C; DCF-1018CP; DCF-1018; DCF-1018P; DCF-1036C; DCF-1036CP; DCF-1036; DCF-1036P

	Exact Configuration
	Confirm one listed configuration during RFQ review

	Destination Requirements
	To be confirmed


ENGINEERING TABLES
DCF-SERIES-MINI-UPS · Complete Model Specifications — DCF-1018C | DCF-1018CP | DCF-1018 | DCF-1018P
	Parameter
	DCF-1018C
	DCF-1018CP
	DCF-1018
	DCF-1018P

	Rated capacity
	18W
	18W
	18W
	18W

	Battery configuration
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell

	Dimensions
	186×114×37mm
	186×114×37mm
	186×114×37mm
	186×114×37mm

	Net weight
	0.45kg
	0.47kg
	0.44kg
	0.47kg

	Transfer time
	Not provided
	Not provided
	Not provided
	Not provided

	Efficiency
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%

	Model configuration — Rated capacity
	18W
	18W
	18W
	18W

	Model configuration — Battery configuration
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell

	Model configuration — Product dimensions
	186×114×37mm
	186×114×37mm
	186×114×37mm
	186×114×37mm

	Model configuration — Net weight
	0.45kg
	0.47kg
	0.44kg
	0.47kg

	Model configuration — Efficiency
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%

	Input — Input voltage
	85–265VAC
	85–265VAC
	85–265VAC
	85–265VAC

	Input — Input frequency
	50–60Hz
	50–60Hz
	50–60Hz
	50–60Hz

	Battery — Battery chemistry
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4

	Battery — Battery cell size
	18650
	18650
	18650
	18650

	Battery — Cell capacity
	2000–2600mAh
	2000–2600mAh
	2000–2600mAh
	2000–2600mAh

	Battery — Battery quantity
	4
	4
	4
	4

	Protection — Protection function
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit

	Environment — Operating temperature
	0–40°C
	0–40°C
	0–40°C
	0–40°C

	Environment — Storage temperature
	-10–70°C
	-10–70°C
	-10–70°C
	-10–70°C

	Environment — Relative humidity
	10–90% RH
	10–90% RH
	10–90% RH
	10–90% RH

	Environment — Altitude
	<3000m
	<3000m
	<3000m
	<3000m

	Environment — Noise level
	<30dB
	<30dB
	<30dB
	<30dB

	Housing — Housing material
	ABS + PC
	ABS + PC
	ABS + PC
	ABS + PC

	Housing — Housing color
	Silver white / Silver gray
	Silver white / Silver gray
	Silver white / Silver gray
	Silver white / Silver gray

	Output — USB output
	5V/2A
	5V/2A
	5V/2A
	5V/2A

	Output — DC output
	9V(12V)/1A
	9V(12V)/1A
	5V/2A; 9V/1A; 12V/1A
	5V/2A; 9V/1A; 12V/1A

	Physical — Package dimensions
	210×170×45mm
	210×170×45mm
	210×170×45mm
	210×170×45mm

	Physical — Gross weight
	0.58kg
	0.6kg
	0.57kg
	0.59kg

	Output — PoE output
	Not provided
	15V/0.6A; 24V/0.6A
	Not provided
	15V/0.6A; 24V/0.6A


DCF-SERIES-MINI-UPS · Complete Model Specifications — DCF-1036C | DCF-1036CP | DCF-1036 | DCF-1036P
	Parameter
	DCF-1036C
	DCF-1036CP
	DCF-1036
	DCF-1036P

	Rated capacity
	36W
	36W
	36W
	36W

	Battery configuration
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell

	Dimensions
	186×114×37mm
	186×114×37mm
	186×114×37mm
	186×114×37mm

	Net weight
	0.52kg
	0.54kg
	0.5kg
	0.54kg

	Transfer time
	Not provided
	Not provided
	Not provided
	Not provided

	Efficiency
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%

	Model configuration — Rated capacity
	36W
	36W
	36W
	36W

	Model configuration — Battery configuration
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell

	Model configuration — Product dimensions
	186×114×37mm
	186×114×37mm
	186×114×37mm
	186×114×37mm

	Model configuration — Net weight
	0.52kg
	0.54kg
	0.5kg
	0.54kg

	Model configuration — Efficiency
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%

	Input — Input voltage
	85–265VAC
	85–265VAC
	85–265VAC
	85–265VAC

	Input — Input frequency
	50–60Hz
	50–60Hz
	50–60Hz
	50–60Hz

	Battery — Battery chemistry
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4

	Battery — Battery cell size
	18650
	18650
	18650
	18650

	Battery — Cell capacity
	2000–2600mAh
	2000–2600mAh
	2000–2600mAh
	2000–2600mAh

	Battery — Battery quantity
	4
	4
	4
	4

	Protection — Protection function
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit

	Environment — Operating temperature
	0–40°C
	0–40°C
	0–40°C
	0–40°C

	Environment — Storage temperature
	-10–70°C
	-10–70°C
	-10–70°C
	-10–70°C

	Environment — Relative humidity
	10–90% RH
	10–90% RH
	10–90% RH
	10–90% RH

	Environment — Altitude
	<3000m
	<3000m
	<3000m
	<3000m

	Environment — Noise level
	<30dB
	<30dB
	<30dB
	<30dB

	Housing — Housing material
	ABS + PC
	ABS + PC
	ABS + PC
	ABS + PC

	Housing — Housing color
	Silver white / Silver gray
	Silver white / Silver gray
	Silver white / Silver gray
	Silver white / Silver gray

	Output — USB output
	5V/2A
	5V/2A
	5V/2A
	5V/2A

	Output — DC output
	9V/12V (3A)
	9V/12V (3A)
	5V/2A; 9V/2A; 12V/2A
	5V/2A; 9V/2A; 12V/2A

	Physical — Package dimensions
	210×170×45mm
	210×170×45mm
	210×170×45mm
	210×170×45mm

	Physical — Gross weight
	0.65kg
	0.67kg
	0.64kg
	0.67kg

	Output — PoE output
	Not provided
	15V/1A; 24V/1A
	Not provided
	15V/1A; 24V/1A
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