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UPS UNINTERRUPTIBLE POWER SUPPLY
VRLA Maintenance-Free Battery Series
Exact model: NX-UP-BA-001
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PRODUCT OVERVIEW
VRLA AGM maintenance-free batteries in 6V and 12V, from 1.2AH to 200AH. 21 models for UPS systems, emergency backup, and power applications.
	Product line
	UPS Uninterruptible Power Supply

	Series / family
	Standalone model

	Exact model
	NX-UP-BA-001

	Applications
	Uninterruptible Power Supply (UPS), Electric Power Systems (EPS), Emergency backup systems, Emergency lighting, Railway and aircraft signals, Alarm and security systems


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Topology
	Power Range
	Phase

	NX-UP-BA-001
	VRLA Maintenance-Free Battery Series
	N/A (Battery)
	1.2AH-200AH (6V and 12V)
	N/A input / N/A output


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Topology
	N/A (Battery)

	Power Range
	1.2AH-200AH (6V and 12V)

	Phase
	N/A input / N/A output

	Form Factor
	Battery Block

	Waveform
	N/A

	Power Factor
	N/A

	Battery Types
	VRLA AGM maintenance-free

	SKU
	NX-UP-BA-001

	Available Configurations
	NP6V1.2AH; NP6V4AH; NP6V4.5AH; NP6V7AH; NP6V10AH; NP12V1.2AH; NP12V2.3AH; NP12V3.4AH; NP12V4AH; NP12V4.5AH; NP12V7AH; NP12V9AH; NP12V12AH; NP12V17AH; NP12V24AH; NP12V38AH; NP12V65AH; NP12V100AH; NP12V120AH; NP12V150AH; NP12V200AH

	Exact Configuration
	Confirm one listed configuration during RFQ review

	Destination Requirements
	To be confirmed


ENGINEERING TABLES
NX-UP-BA-001 · Complete Model Specifications — NP6V1.2AH | NP6V4AH | NP6V4.5AH | NP6V7AH
	Parameter
	NP6V1.2AH
	NP6V4AH
	NP6V4.5AH
	NP6V7AH

	Rated capacity
	6V / 1.2AH
	6V / 4AH
	6V / 4.5AH
	6V / 7AH

	Battery configuration
	6V / 1.2AH
	6V / 4AH
	6V / 4.5AH
	6V / 7AH

	Dimensions
	Not provided
	Not provided
	Not provided
	Not provided

	Net weight
	Not provided
	Not provided
	Not provided
	Not provided

	Transfer time
	Not provided
	Not provided
	Not provided
	Not provided

	Efficiency
	Not provided
	Not provided
	Not provided
	Not provided

	Model configuration — Rated capacity
	6V / 1.2AH
	6V / 4AH
	6V / 4.5AH
	6V / 7AH

	Model configuration — Battery configuration
	6V / 1.2AH
	6V / 4AH
	6V / 4.5AH
	6V / 7AH

	Battery — Battery technology
	VRLA AGM
	VRLA AGM
	VRLA AGM
	VRLA AGM

	Battery — Capacity reference temperature
	25°C
	25°C
	25°C
	25°C

	Battery — Discharge endpoint
	1.75V/cell
	1.75V/cell
	1.75V/cell
	1.75V/cell

	Battery — 20h capacity at 25°C / 1.75V per cell
	1.2Ah
	Not provided
	4.5Ah
	Not provided

	Battery — 10h capacity at 25°C / 1.75V per cell
	1.1Ah
	Not provided
	4Ah
	Not provided

	Physical — Length
	97mm ±1mm
	Not provided
	70mm ±1mm
	Not provided

	Physical — Width
	25mm ±1mm
	Not provided
	47mm ±1mm
	Not provided

	Physical — Body height
	52mm ±2mm
	Not provided
	102mm ±2mm
	Not provided

	Physical — Overall height
	58mm ±2mm
	Not provided
	105mm ±2mm
	Not provided

	Physical — Terminal type
	E
	Not provided
	E
	Not provided


NX-UP-BA-001 · Complete Model Specifications — NP6V10AH | NP12V1.2AH | NP12V2.3AH | NP12V3.4AH
	Parameter
	NP6V10AH
	NP12V1.2AH
	NP12V2.3AH
	NP12V3.4AH

	Rated capacity
	6V / 10AH
	12V / 1.2AH
	12V / 2.3AH
	12V / 3.4AH

	Battery configuration
	6V / 10AH
	12V / 1.2AH
	12V / 2.3AH
	12V / 3.4AH

	Dimensions
	Not provided
	Not provided
	Not provided
	Not provided

	Net weight
	Not provided
	Not provided
	Not provided
	Not provided

	Transfer time
	Not provided
	Not provided
	Not provided
	Not provided

	Efficiency
	Not provided
	Not provided
	Not provided
	Not provided

	Model configuration — Rated capacity
	6V / 10AH
	12V / 1.2AH
	12V / 2.3AH
	12V / 3.4AH

	Model configuration — Battery configuration
	6V / 10AH
	12V / 1.2AH
	12V / 2.3AH
	12V / 3.4AH

	Battery — Battery technology
	VRLA AGM
	VRLA AGM
	VRLA AGM
	VRLA AGM

	Battery — Capacity reference temperature
	25°C
	25°C
	25°C
	25°C

	Battery — Discharge endpoint
	1.75V/cell
	1.75V/cell
	1.75V/cell
	1.75V/cell

	Battery — 20h capacity at 25°C / 1.75V per cell
	10Ah
	1.2Ah
	Not provided
	Not provided

	Battery — 10h capacity at 25°C / 1.75V per cell
	9.3Ah
	1.1Ah
	Not provided
	Not provided

	Physical — Length
	151mm ±1mm
	97mm ±1mm
	Not provided
	Not provided

	Physical — Width
	50mm ±1mm
	48mm ±1mm
	Not provided
	Not provided

	Physical — Body height
	94mm ±2mm
	52mm ±2mm
	Not provided
	Not provided

	Physical — Overall height
	98mm ±2mm
	58mm ±2mm
	Not provided
	Not provided

	Physical — Terminal type
	E
	E
	Not provided
	Not provided


NX-UP-BA-001 · Complete Model Specifications — NP12V4AH | NP12V4.5AH | NP12V7AH | NP12V9AH
	Parameter
	NP12V4AH
	NP12V4.5AH
	NP12V7AH
	NP12V9AH

	Rated capacity
	12V / 4AH
	12V / 4.5AH
	12V / 7AH
	12V / 9AH

	Battery configuration
	12V / 4AH
	12V / 4.5AH
	12V / 7AH
	12V / 9AH

	Dimensions
	Not provided
	Not provided
	Not provided
	Not provided

	Net weight
	Not provided
	Not provided
	Not provided
	Not provided

	Transfer time
	Not provided
	Not provided
	Not provided
	Not provided

	Efficiency
	Not provided
	Not provided
	Not provided
	Not provided

	Model configuration — Rated capacity
	12V / 4AH
	12V / 4.5AH
	12V / 7AH
	12V / 9AH

	Model configuration — Battery configuration
	12V / 4AH
	12V / 4.5AH
	12V / 7AH
	12V / 9AH

	Battery — Battery technology
	VRLA AGM
	VRLA AGM
	VRLA AGM
	VRLA AGM

	Battery — Capacity reference temperature
	25°C
	25°C
	25°C
	25°C

	Battery — Discharge endpoint
	1.75V/cell
	1.75V/cell
	1.75V/cell
	1.75V/cell

	Battery — 20h capacity at 25°C / 1.75V per cell
	Not provided
	4.5Ah
	7.5Ah
	Not provided

	Battery — 10h capacity at 25°C / 1.75V per cell
	Not provided
	4.1Ah
	7Ah
	Not provided

	Physical — Length
	Not provided
	90mm ±1mm
	151mm ±1mm
	Not provided

	Physical — Width
	Not provided
	70mm ±1mm
	65mm ±1mm
	Not provided

	Physical — Body height
	Not provided
	102mm ±2mm
	94mm ±2mm
	Not provided

	Physical — Overall height
	Not provided
	105mm ±2mm
	98mm ±2mm
	Not provided

	Physical — Terminal type
	Not provided
	E
	E
	Not provided


NX-UP-BA-001 · Complete Model Specifications — NP12V12AH | NP12V17AH | NP12V24AH | NP12V38AH
	Parameter
	NP12V12AH
	NP12V17AH
	NP12V24AH
	NP12V38AH

	Rated capacity
	12V / 12AH
	12V / 17AH
	12V / 24AH
	12V / 38AH

	Battery configuration
	12V / 12AH
	12V / 17AH
	12V / 24AH
	12V / 38AH

	Dimensions
	Not provided
	Not provided
	Not provided
	Not provided

	Net weight
	Not provided
	Not provided
	Not provided
	Not provided

	Transfer time
	Not provided
	Not provided
	Not provided
	Not provided

	Efficiency
	Not provided
	Not provided
	Not provided
	Not provided

	Model configuration — Rated capacity
	12V / 12AH
	12V / 17AH
	12V / 24AH
	12V / 38AH

	Model configuration — Battery configuration
	12V / 12AH
	12V / 17AH
	12V / 24AH
	12V / 38AH

	Battery — Battery technology
	VRLA AGM
	VRLA AGM
	VRLA AGM
	VRLA AGM

	Battery — Capacity reference temperature
	25°C
	25°C
	25°C
	25°C

	Battery — Discharge endpoint
	1.75V/cell
	1.75V/cell
	1.75V/cell
	1.75V/cell

	Battery — 20h capacity at 25°C / 1.75V per cell
	12Ah
	17Ah
	Requires confirmation
	41Ah

	Battery — 10h capacity at 25°C / 1.75V per cell
	11.1Ah
	15.8Ah
	24Ah
	38Ah

	Physical — Length
	151mm ±1mm
	181mm ±1mm
	166mm ±1mm
	197mm ±1mm

	Physical — Width
	98mm ±1mm
	76mm ±1mm
	125mm ±1mm
	165mm ±1mm

	Physical — Body height
	98mm ±2mm
	167mm ±2mm
	175mm ±2mm
	170mm ±2mm

	Physical — Overall height
	101mm ±2mm
	125mm ±2mm
	175mm ±2mm
	170mm ±2mm

	Physical — Terminal type
	E
	G
	G
	G


NX-UP-BA-001 · Complete Model Specifications — NP12V65AH | NP12V100AH | NP12V120AH | NP12V150AH
	Parameter
	NP12V65AH
	NP12V100AH
	NP12V120AH
	NP12V150AH

	Rated capacity
	12V / 65AH
	12V / 100AH
	12V / 120AH
	12V / 150AH

	Battery configuration
	12V / 65AH
	12V / 100AH
	12V / 120AH
	12V / 150AH

	Dimensions
	Not provided
	Not provided
	Not provided
	Not provided

	Net weight
	Not provided
	Not provided
	Not provided
	Not provided

	Transfer time
	Not provided
	Not provided
	Not provided
	Not provided

	Efficiency
	Not provided
	Not provided
	Not provided
	Not provided

	Model configuration — Rated capacity
	12V / 65AH
	12V / 100AH
	12V / 120AH
	12V / 150AH

	Model configuration — Battery configuration
	12V / 65AH
	12V / 100AH
	12V / 120AH
	12V / 150AH

	Battery — Battery technology
	VRLA AGM
	VRLA AGM
	VRLA AGM
	VRLA AGM

	Battery — Capacity reference temperature
	25°C
	25°C
	25°C
	25°C

	Battery — Discharge endpoint
	1.75V/cell
	1.75V/cell
	1.75V/cell
	1.75V/cell

	Battery — 20h capacity at 25°C / 1.75V per cell
	70Ah
	100Ah
	150Ah
	Not provided

	Battery — 10h capacity at 25°C / 1.75V per cell
	65Ah
	93Ah
	110Ah
	Not provided

	Physical — Length
	350mm ±1mm
	400mm ±1mm
	405mm ±1mm
	Not provided

	Physical — Width
	174mm ±1mm
	172mm ±1mm
	172mm ±1mm
	Not provided

	Physical — Body height
	174mm ±2mm
	215mm ±2mm
	210mm ±2mm
	Not provided

	Physical — Overall height
	174mm ±2mm
	243mm ±2mm
	240mm ±2mm
	Not provided

	Physical — Terminal type
	G
	G
	G
	Not provided


NX-UP-BA-001 · Complete Model Specifications — NP12V200AH
	Parameter
	NP12V200AH

	Rated capacity
	12V / 200AH

	Battery configuration
	12V / 200AH

	Dimensions
	Not provided

	Net weight
	Not provided

	Transfer time
	Not provided

	Efficiency
	Not provided

	Model configuration — Rated capacity
	12V / 200AH

	Model configuration — Battery configuration
	12V / 200AH

	Battery — Battery technology
	VRLA AGM

	Battery — Capacity reference temperature
	25°C

	Battery — Discharge endpoint
	1.75V/cell

	Battery — 20h capacity at 25°C / 1.75V per cell
	218Ah

	Battery — 10h capacity at 25°C / 1.75V per cell
	200Ah

	Physical — Length
	524mm ±1mm

	Physical — Width
	216mm ±1mm

	Physical — Body height
	216mm ±2mm

	Physical — Overall height
	244mm ±2mm

	Physical — Terminal type
	G
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Voltage 25°C (AH) Size terminals
) 20HR 10HR KL+1 W1 fH2 fEH2
1.75V/CELL | 1.75V/CELL ~ (MM) (MM) (MM) (MM)
NP6V1.2AH 6 1.2 1.1 97 25 52 58 E
NP6V4.5AH 6 4.5 4 70 47 102 105 E
NP6V8AH 6 8 7.4 151 50 94 98 E
NP6V10AH 6 10 93 151 50 94 98 E
NP12V1.2AH 12 1.2 1.1 97 48 52 58 E
NP12V2.0AH 12 2 1.9 178 34 60 64 E
NP12V4.5AH 12 45 4.1 90 70 102 105 E
NP5V12AH 12 5 46 90 70 102 105 E
NP12V7AH 12 7.5 7.0 151 65 94 98 E
NP12V8AH 12 8 7.5 151 65 94 98 E
NP12V12AH 12 12 111 151 98 98 101 E
NP12V14AH 12 14 13 151 98 98 101 E
NP12V17AH 12 17 15.8 181 76 167 125 G
NP12V24AH 12 26 24 166 125 175 175 G
NP12V30AH 12 30 28 166 175 175 175 G
NP12V38AH 12 41 38 197 165 170 170 G
NP12V55AH 12 55 51 236 205 205 239 G
NP12V65AH 12 70 65 350 174 174 174 G
NP12V100AH 12 100 93 400 172 215 243 G
NP12V120AH 12 150 110 405 172 210 240 G
NF12Y150AH 12 160 150 480 172 240 240 G
NP12V180AH 12 200 186 524 216 216 244 G
NP12V200AH 12 218 200 524 216 216 244 G
NP12V250AH 12 262 250 522 268 220 225 G
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