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	PRODUCT SPECIFICATION
DC Mini UPS 18W-36W Series
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UPS UNINTERRUPTIBLE POWER SUPPLY
DC Mini UPS 18W-36W Series
Exact model: NX-UP-DC-001
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PRODUCT OVERVIEW
Compact DC Mini UPS series with built-in lithium battery for routers, ONT devices, and small network equipment. Seven model variants from 18W to 36W.
	Product line
	UPS Uninterruptible Power Supply

	Series / family
	Standalone model

	Exact model
	NX-UP-DC-001

	Applications
	Routers and modems, Optical network terminals (ONT), CCTV cameras, Small network equipment, IoT devices


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Topology
	Power Range
	Phase

	NX-UP-DC-001
	DC Mini UPS 18W-36W Series
	DC UPS with Li-ion battery
	18W-36W
	85–265VAC, 50–60Hz input / DC / USB / PoE options output


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Topology
	DC UPS with Li-ion battery

	Power Range
	18W-36W

	Phase
	85–265VAC, 50–60Hz input / DC / USB / PoE options output

	Form Factor
	Compact DC Unit

	Waveform
	DC output

	Power Factor
	N/A (DC output)

	Battery Types
	Lithium-ion / LiFePO4

	SKU
	NX-UP-DC-001

	Available Configurations
	DC1018CP; DC1018; DC1018P; DC1024P; DC1036CP; DC1036; DC1036P

	Exact Configuration
	Confirm one listed configuration during RFQ review

	Destination Requirements
	To be confirmed


ENGINEERING TABLES
NX-UP-DC-001 · Complete Model Specifications — DC1018CP | DC1018 | DC1018P | DC1024P
	Parameter
	DC1018CP
	DC1018
	DC1018P
	DC1024P

	Rated capacity
	18W
	18W
	18W
	24W

	Battery configuration
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell

	Dimensions
	160×105×33mm
	160×105×33mm
	160×105×33mm
	160×105×33mm

	Net weight
	0.38kg
	0.4kg
	0.39kg
	0.4kg

	Transfer time
	Not provided
	Not provided
	Not provided
	Not provided

	Efficiency
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%

	Model configuration — Rated capacity
	18W
	18W
	18W
	24W

	Model configuration — Battery configuration
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell

	Model configuration — Product dimensions
	160×105×33mm
	160×105×33mm
	160×105×33mm
	160×105×33mm

	Model configuration — Net weight
	0.38kg
	0.4kg
	0.39kg
	0.4kg

	Model configuration — Efficiency
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%

	Input — Input voltage
	85–265VAC
	85–265VAC
	85–265VAC
	85–265VAC

	Input — Input frequency
	50–60Hz
	50–60Hz
	50–60Hz
	50–60Hz

	Battery — Battery chemistry
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4

	Battery — Battery cell size
	18650
	18650
	18650
	18650

	Battery — Cell capacity
	2000–2600mAh
	2000–2600mAh
	2000–2600mAh
	2000–2600mAh

	Battery — Battery quantity
	4
	4
	4
	4

	Protection — Protection function
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit

	Environment — Operating temperature
	0–40°C
	0–40°C
	0–40°C
	0–40°C

	Environment — Storage temperature
	-10–70°C
	-10–70°C
	-10–70°C
	-10–70°C

	Environment — Relative humidity
	10–90% RH
	10–90% RH
	10–90% RH
	10–90% RH

	Environment — Altitude
	<3000m
	<3000m
	<3000m
	<3000m

	Environment — Noise level
	<30dB
	<30dB
	<30dB
	<30dB

	Housing — Housing material
	ABS
	ABS
	ABS
	ABS

	Housing — Housing color
	Black / White
	Black / White
	Black / White
	Black / White

	Output — USB output
	5V/2A
	5V/2A
	5V/2A
	5V/2A

	Output — DC output
	9V(12V)/1A
	5V/2A; 9V/1A; 12V/1A
	5V/2A; 9V/1A; 12V/1A
	5V/2A; 9V/2A; 12V/2A

	Output — PoE output
	15V/0.6A; 24V/0.6A
	Not provided
	15V/0.6A; 24V/0.6A
	15V/1A; 24V/1A

	Physical — Package dimensions
	180×160×37mm
	180×160×37mm
	180×160×37mm
	180×160×37mm

	Physical — Gross weight
	0.51kg
	0.53kg
	0.5kg
	0.52kg


NX-UP-DC-001 · Complete Model Specifications — DC1036CP | DC1036 | DC1036P
	Parameter
	DC1036CP
	DC1036
	DC1036P

	Rated capacity
	36W
	36W
	36W

	Battery configuration
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell

	Dimensions
	160×105×33mm
	160×105×33mm
	160×105×33mm

	Net weight
	0.41kg
	0.4kg
	0.42kg

	Transfer time
	Not provided
	Not provided
	Not provided

	Efficiency
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%

	Model configuration — Rated capacity
	36W
	36W
	36W

	Model configuration — Battery configuration
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell
	4 × 18650; 2000–2600mAh/cell

	Model configuration — Product dimensions
	160×105×33mm
	160×105×33mm
	160×105×33mm

	Model configuration — Net weight
	0.41kg
	0.4kg
	0.42kg

	Model configuration — Efficiency
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%

	Input — Input voltage
	85–265VAC
	85–265VAC
	85–265VAC

	Input — Input frequency
	50–60Hz
	50–60Hz
	50–60Hz

	Battery — Battery chemistry
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4

	Battery — Battery cell size
	18650
	18650
	18650

	Battery — Cell capacity
	2000–2600mAh
	2000–2600mAh
	2000–2600mAh

	Battery — Battery quantity
	4
	4
	4

	Protection — Protection function
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit

	Environment — Operating temperature
	0–40°C
	0–40°C
	0–40°C

	Environment — Storage temperature
	-10–70°C
	-10–70°C
	-10–70°C

	Environment — Relative humidity
	10–90% RH
	10–90% RH
	10–90% RH

	Environment — Altitude
	<3000m
	<3000m
	<3000m

	Environment — Noise level
	<30dB
	<30dB
	<30dB

	Housing — Housing material
	ABS
	ABS
	ABS

	Housing — Housing color
	Black / White
	Black / White
	Black / White

	Output — USB output
	5V/2A
	5V/2A
	5V/2A

	Output — DC output
	9V/12V (3A)
	5V/2A; 9V/2A; 12V/2A
	5V/2A; 9V/2A; 12V/2A

	Output — PoE output
	15V/1A; 24V/1A
	Not provided
	15V/1A; 24V/1A

	Physical — Package dimensions
	180×160×37mm
	180×160×37mm
	180×160×37mm

	Physical — Gross weight
	0.55kg
	0.51kg
	0.56kg



	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
	Page 1


image2.png




image3.jpg




image4.jpg
5 Model

i\ HJE Input voltage

it R K T 3R

Maximum output power

i tH L
Output voltage

%% Efficiency

A

Battery specifications
LA 5T

Battery material
A

Battery capacity
GEREE-8T

Battery quantity
bhFeRt

Shell material
Shaeidits
Shell color

PRI T BE

Protection function

174i# I )% Storage temp

R EE Altitude
153 Noise

i

JR5F Product size

En

4% R~} Package size

1§ Net weight

EHGross weight

LAE# % Work temperature

HXHEE Relative humidity

DC1018CP  DC1018 DC1018P DC1024P  DC1036CP DC1036 DC1036P
85-265Vac/50-60Hz
18W 24W 36W
USB 5V/2A | USB 5V/2A | USB 5V/2A | USB 5V/2A USB 5V/2A  USB 5V/2A
av( 133)/1A DC 5V/2A  DC5V/2A DC5V/I2A  USB 5V/2A DC 5VI2A DC 5V/2A
15?//0()FGA DC 9V/1A | DC9V/1A | DC 9V/2A 9V/1[2)$(3A) DC 9V/i2A DC 9V/I2A
24?/%?6A DC 12V/1A DC 12V/1A DC 12V/2A POE 15V/1A  DC 12V/I2A  DC 12Vi2A
15?/(/)0I.56A 12\(/:;I‘IEA POE 24V/1A POE 15V/1A
L = POE 24V/1A

24V/I0.6A  24V/1A

AC mode:>85%, Tii Hifi simunicipal power mode: >85%, Fijtifi{Battery mode:>90%

18650

= IR AW R #Lithium-lon battery/LiFePO4 battery

2000mah~2600mah

ABS

B, A GESCRERD
Black. White (Provide color customization)

AR RS WA SR SRR R

Over-charge,over-discharge,over-current,overload,over-temperature and short circuit protection
0C-40C
-10°C-70C
10%-90%RH
<3000m
<30db
160*105*33mm
180*160*37mm
0.38kg 0.4kg 0.39g 0.4kg 0.41kg 0.4kg 0.42kg

0.51kg 0.53kg 0.5kg 0.52kg 0.55kg 0.51kg 0.56kg




image1.png








