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DC Mini UPS 45W-120W Series


[image: ]
UPS UNINTERRUPTIBLE POWER SUPPLY
DC Mini UPS 45W-120W Series
Exact model: NX-UP-DC-002
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PRODUCT OVERVIEW
Higher-power DC Mini UPS series with POE support for CCTV cameras, network equipment, and multi-voltage devices. Four model variants from 45W to 120W.
	Product line
	UPS Uninterruptible Power Supply

	Series / family
	Standalone model

	Exact model
	NX-UP-DC-002

	Applications
	CCTV systems, Routers and network terminals, POE-powered devices, Multi-voltage small equipment


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Topology
	Power Range
	Phase

	NX-UP-DC-002
	DC Mini UPS 45W-120W Series
	DC UPS with Li-ion battery & POE
	45W-120W
	100–240VAC, 50–60Hz input / DC / USB / PoE options output


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Topology
	DC UPS with Li-ion battery & POE

	Power Range
	45W-120W

	Phase
	100–240VAC, 50–60Hz input / DC / USB / PoE options output

	Form Factor
	Compact DC Unit

	Waveform
	DC output

	Power Factor
	N/A (DC output)

	Battery Types
	Lithium-ion / LiFePO4

	SKU
	NX-UP-DC-002

	Available Configurations
	DCP-045W; DCP-60W; DCP-100W; DCP-120W

	Exact Configuration
	Confirm one listed configuration during RFQ review

	Destination Requirements
	To be confirmed


ENGINEERING TABLES
NX-UP-DC-002 · Complete Model Specifications — DCP-045W | DCP-60W | DCP-100W | DCP-120W
	Parameter
	DCP-045W
	DCP-60W
	DCP-100W
	DCP-120W

	Rated capacity
	45W
	60W
	100W
	120W

	Battery configuration
	4 / 8 cells; 18650
	4 / 8 cells; 18650 / 32650
	4 / 8 cells; 18650 / 32650
	4 / 8 cells; 18650 / 32650

	Dimensions
	180×130×64mm
	214×158.5×86mm
	214×158.5×86mm
	214×158.5×86mm

	Net weight
	0.83kg
	1.85kg
	1.88kg
	1.9kg

	Transfer time
	Not provided
	Not provided
	Not provided
	Not provided

	Efficiency
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%

	Model configuration — Rated capacity
	45W
	60W
	100W
	120W

	Model configuration — Battery configuration
	4 / 8 cells; 18650
	4 / 8 cells; 18650 / 32650
	4 / 8 cells; 18650 / 32650
	4 / 8 cells; 18650 / 32650

	Model configuration — Product dimensions
	180×130×64mm
	214×158.5×86mm
	214×158.5×86mm
	214×158.5×86mm

	Model configuration — Net weight
	0.83kg
	1.85kg
	1.88kg
	1.9kg

	Model configuration — Efficiency
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%
	AC >85%; Battery >90%

	Input — Input voltage
	100–240VAC
	100–240VAC
	100–240VAC
	100–240VAC

	Input — Input frequency
	50–60Hz
	50–60Hz
	50–60Hz
	50–60Hz

	Battery — Battery chemistry
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4
	Lithium-ion / LiFePO4

	Battery — Battery quantity
	4 / 8
	4 / 8
	4 / 8
	4 / 8

	Battery — Battery cell size
	18650
	18650 / 32650
	18650 / 32650
	18650 / 32650

	Battery — Cell capacity
	2000–2600mAh
	2000–6000mAh
	2000–6000mAh
	2000–6000mAh

	Protection — Protection function
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit
	Over-charge, over-discharge, over-current, overload, over-temperature and short circuit

	Environment — Operating temperature
	0–40°C
	0–40°C
	0–40°C
	0–40°C

	Environment — Storage temperature
	-10–70°C
	-10–70°C
	-10–70°C
	-10–70°C

	Environment — Relative humidity
	10–90% RH
	10–90% RH
	10–90% RH
	10–90% RH

	Environment — Altitude
	<3000m
	<3000m
	<3000m
	<3000m

	Environment — Noise level
	<30dB
	<30dB
	<30dB
	<30dB

	Housing — Housing material
	ABS
	ABS
	ABS
	ABS

	Housing — Housing color
	Black / White
	Black / White
	Black / White
	Black / White

	Output — USB output
	5V/2.4A
	5V/2.4A
	5V/2.4A
	5V/2.4A

	Output — DC 5V output
	5V/2.4A
	5V/2.4A
	5V/2.4A
	5V/2.4A

	Output — DC 9V / 12V output
	9V(12V)/2A
	9V(12V)/2A
	9V(12V)/2A
	9V(12V)/2A

	Output — DC 12V output
	12V/3.5A
	12V/5A
	12V/8A
	12V/10A

	Output — PoE 15V output
	15V/1.5A
	Not provided
	15V/1.5A
	15V/1.5A

	Output — PoE 24V output
	24V/1A
	24V/1A
	24V/1A
	24V/1A

	Output — PoE 48V output
	48V/0.6A
	48V/0.6A (optional)
	48V/0.6A (optional)
	48V/0.6A (optional)

	Physical — Package dimensions
	195×180×70mm
	230×230×95mm
	230×230×95mm
	230×230×95mm

	Physical — Gross weight
	1.2kg
	2.6kg
	2.63kg
	2.65kg

	Output — DC 19V output
	Not provided
	19V/3A
	19V/5A
	19V/6A
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