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UPS UNINTERRUPTIBLE POWER SUPPLY
Standby UPS 650VA-3000VA Series
Exact model: NX-UP-ST-001
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PRODUCT OVERVIEW
Cost-effective offline UPS series providing reliable battery backup and surge protection for personal computers, POS systems, and small office equipment. Available in 650VA to 3000VA capacities.
	Product line
	UPS Uninterruptible Power Supply

	Series / family
	Standalone model

	Exact model
	NX-UP-ST-001

	Applications
	Personal computers, Printers, POS terminals, Security systems, Fax machines, Modems and routers


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Topology
	Power Range
	Phase

	NX-UP-ST-001
	Standby UPS 650VA-3000VA Series
	Offline (Standby)
	650VA-3000VA / 390W-1800W
	Single phase input / Single phase output


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Topology
	Offline (Standby)

	Power Range
	650VA-3000VA / 390W-1800W

	Phase
	Single phase input / Single phase output

	Form Factor
	Tower

	Waveform
	Simulated sine wave

	Power Factor
	0.6

	Battery Types
	VRLA sealed lead-acid

	SKU
	NX-UP-ST-001

	Available Configurations
	SP650; SP1000; SP1500; SP2000; SP3000

	Exact Configuration
	Confirm one listed configuration during RFQ review

	Destination Requirements
	To be confirmed


ENGINEERING TABLES
NX-UP-ST-001 · Complete Model Specifications — SP650 | SP1000 | SP1500 | SP2000
	Parameter
	SP650
	SP1000
	SP1500
	SP2000

	Rated capacity
	650VA / 390W
	1000VA / 600W
	1500VA / 900W
	2000VA / 1200W

	Battery configuration
	12V/7AH × 1
	12V/9AH × 1
	12V/9AH × 2
	12V/9AH × 2

	Dimensions
	320×90×140mm
	320×90×140mm
	350×115×275mm
	350×115×275mm

	Net weight
	5.1kg
	5.7kg
	12.2kg
	12.35kg

	Transfer time
	≤6ms
	≤6ms
	≤6ms
	≤6ms

	Efficiency
	Not provided
	Not provided
	Not provided
	Not provided

	Model configuration — Rated capacity
	650VA / 390W
	1000VA / 600W
	1500VA / 900W
	2000VA / 1200W

	Model configuration — Battery configuration
	12V/7AH × 1
	12V/9AH × 1
	12V/9AH × 2
	12V/9AH × 2

	Model configuration — Product dimensions
	320×90×140mm
	320×90×140mm
	350×115×275mm
	350×115×275mm

	Model configuration — Net weight
	5.1kg
	5.7kg
	12.2kg
	12.35kg

	Model configuration — Transfer time
	≤6ms
	≤6ms
	≤6ms
	≤6ms

	Input — Input voltage range
	140–280VAC
	140–280VAC
	140–280VAC
	140–280VAC

	Input — Input frequency
	50Hz; tolerance requires confirmation
	50Hz; tolerance requires confirmation
	50Hz; tolerance requires confirmation
	50Hz; tolerance requires confirmation

	Output — Voltage regulation
	±10%
	±10%
	±10%
	±10%

	Output — Output frequency
	50Hz; tolerance requires confirmation
	50Hz; tolerance requires confirmation
	50Hz; tolerance requires confirmation
	50Hz; tolerance requires confirmation

	Charging — Charging time
	10–16h to 90% capacity
	10–16h to 90% capacity
	10–16h to 90% capacity
	10–16h to 90% capacity

	Protection — Protection function
	Discharge, short circuit and overload
	Discharge, short circuit and overload
	Discharge, short circuit and overload
	Discharge, short circuit and overload

	Display & Alarms — Display
	LCD
	LCD
	LCD
	LCD

	Display & Alarms — Battery mode alarm
	Every 4 seconds
	Every 4 seconds
	Every 4 seconds
	Every 4 seconds

	Display & Alarms — Low battery alarm
	Every second
	Every second
	Every second
	Every second

	Display & Alarms — Overload alarm
	Every second
	Every second
	Every second
	Every second

	Display & Alarms — Fault alarm
	Continuous
	Continuous
	Continuous
	Continuous

	Environment — Operating temperature
	0–40°C
	0–40°C
	0–40°C
	0–40°C

	Environment — Relative humidity
	0–90% RH
	0–90% RH
	0–90% RH
	0–90% RH

	Environment — Noise level
	<40dB
	<40dB
	<40dB
	<40dB


NX-UP-ST-001 · Complete Model Specifications — SP3000
	Parameter
	SP3000

	Rated capacity
	3000VA / 1800W

	Battery configuration
	12V/12AH × 2

	Dimensions
	350×115×275mm

	Net weight
	15.8kg

	Transfer time
	≤6ms

	Efficiency
	Not provided

	Model configuration — Rated capacity
	3000VA / 1800W

	Model configuration — Battery configuration
	12V/12AH × 2

	Model configuration — Product dimensions
	350×115×275mm

	Model configuration — Net weight
	15.8kg

	Model configuration — Transfer time
	≤6ms

	Input — Input voltage range
	140–280VAC

	Input — Input frequency
	50Hz; tolerance requires confirmation

	Output — Voltage regulation
	±10%

	Output — Output frequency
	50Hz; tolerance requires confirmation

	Charging — Charging time
	10–16h to 90% capacity

	Protection — Protection function
	Discharge, short circuit and overload

	Display & Alarms — Display
	LCD

	Display & Alarms — Battery mode alarm
	Every 4 seconds

	Display & Alarms — Low battery alarm
	Every second

	Display & Alarms — Overload alarm
	Every second

	Display & Alarms — Fault alarm
	Continuous

	Environment — Operating temperature
	0–40°C

	Environment — Relative humidity
	0–90% RH

	Environment — Noise level
	<40dB



	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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