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VIDEO WALL DISPLAY & NETWORK DECODING SYSTEM
55-inch LCD Video Wall Panel for Control Room Display
Exact model: NX-VP-5535
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PRODUCT OVERVIEW
A 55-inch Full HD LCD panel with a 3.5 mm combined bezel, designed for tiled monitoring, command and presentation walls.
	Product line
	Video Wall Display & Network Decoding System

	Series / family
	Standalone model

	Exact model
	NX-VP-5535

	Applications
	Security control room, Command center, Monitoring center, Presentation wall


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Panel size
	Combined bezel
	Resolution

	NX-VP-5535
	55-inch LCD Video Wall Panel for Control Room Display
	55 inches
	3.5 mm
	1920 × 1080


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Panel size
	55 inches

	Combined bezel
	3.5 mm

	Resolution
	1920 × 1080

	Brightness
	400 nit typical

	Viewing angle
	178° H / V; 178° horizontal / vertical

	Power
	Up to 150 W

	Contrast ratio
	1200:1 typical

	Response time
	8 ms typical

	Backlight
	D-LED

	Dimensions
	1213.5 × 684.3 × 89.94 mm

	Net weight
	14.4 kg

	Power consumption
	Up to 150 W

	Mounting review
	Confirm wall, cabinet or front-maintenance structure from the approved project drawing


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Security control room
Command center
Monitoring center
Presentation wall
	Confirm rows × columns, mounting method, maintenance access and packing before quotation.
Color calibration, controller compatibility and final interfaces must be checked against the approved project submittal.


Project supply: MOQ — Project-based; confirm from wall layout and quantity · Lead time — Confirm after layout, mounting and packing review · FOB port — China main ports · OEM/ODM — Available; confirm project scope
PROJECT CONFIGURATION CHECKLIST
	Exact model
	NX-VP-5535

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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