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VIDEO WALL DISPLAY & NETWORK DECODING SYSTEM
5-inch Network PTZ Control Keyboard
Exact model: NX-PC-5S3
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PRODUCT OVERVIEW
A network PTZ control keyboard with a 5-inch display, four-axis joystick, video decoding and PoE support for surveillance operators.
	Product line
	Video Wall Display & Network Decoding System

	Series / family
	Standalone model

	Exact model
	NX-PC-5S3

	Applications
	Security operator desk, PTZ camera control, Monitoring center, Decoder operation


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Display
	Managed devices
	Decoding

	NX-PC-5S3
	5-inch Network PTZ Control Keyboard
	5-inch 800 × 480
	Up to 999
	1080p at 30 fps


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Display
	5-inch 800 × 480 TFT LCD

	Managed devices
	Up to 999

	Decoding
	1080p at 30 fps

	Interfaces
	RJ45 / RS422 / RS232; RJ45, RS422 and RS232

	Power
	DC 12 V / PoE

	Consumption
	Up to 5 W

	Operating system
	Linux

	Video decoding
	H.265 / H.264, up to 1080p at 30 fps

	Control
	Four-axis variable-speed joystick

	Power consumption
	Up to 5 W

	Operating temperature
	-10 to 55 °C


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Security operator desk
PTZ camera control
Monitoring center
Decoder operation
	Confirm camera brands/models, protocol, device count and required serial interfaces before quotation.


Project supply: MOQ — Confirm by project quantity · Lead time — Confirm after compatibility review · FOB port — China main ports · OEM/ODM — Available; confirm project scope
PROJECT CONFIGURATION CHECKLIST
	Exact model
	NX-PC-5S3

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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