NexPro PT736X-2MP/5MP

NexPro PTZ 36X-2MP/5MP 

7-Inch 5MP 36× Optical Zoom Intelligent High-Speed PTZ Camera
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Professional-Grade 7-Inch High-Speed PTZ — Built for Perimeter Surveillance, Industrial Compounds & Large Outdoor Areas
The NexPro PT736X-5MP combines a 5-megapixel ultra-low-light CMOS sensor with a powerful 36× optical zoom lens and 150-meter infrared reach in a weatherproof IP66 housing. Advanced 2D/3D noise reduction and AE exposure algorithms keep night footage clean and usable. Full ONVIF Profile S compliance ensures seamless integration with leading NVR platforms, while Seetong Client and Seetong APP provide instant mobile and desktop access via Seetong Cloud. An open SDK (Linux/Windows) and CGI protocol enable rapid secondary development for custom project requirements.
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	Topology 1
	IPC — NVR — Seetong Cloud — Seetong Client

	Topology 2
	IPC — NVR — Seetong Client

	Topology 3
	IPC — NVR — Seetong Cloud — Seetong APP

	Topology 4
	IPC — Seetong Client (Direct)

	Topology 5
	IPC — Seetong Cloud — Seetong APP


Core Highlights
	5MP @ 30fps
	36× Optical Zoom
	150m IR
	IP66

	2592×1944 max resolution with smooth 30fps
	f=4.6~167mm, F1.6~F4.8, 2.3°~61.2° FOV
	Φ42 8-LED array, up to 150m night vision
	Outdoor-rated, -40°C to +60°C operating range
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Technical Specifications
	No.
	Parameter
	NexPro PT736X-2MP
	NexPro PT736X-5MP

	1
	Image Sensor
	1/2.8" SONY IMX 307
	1/3" HiSilicon 3516A + SONY 3335

	2
	Video Compression
	H.265 Main Profile / H.264 High Profile / M-JPEG
	H.265 Main Profile / H.264 High Profile / M-JPEG

	3
	Max Resolution
	1080P (1920×1080)
	5MP (2592×1944)

	4
	Effective Pixels
	2.0 Megapixels
	5.0 Megapixels

	5
	Video Resolution
	1920×1080 @ 30fps; 1280×720 @ 60fps
	2592×1944 @ 30fps; 2592×1520 @ 30fps; 2304×1296 @ 30fps; 1920×1080 @ 30fps

	6
	Lens
	36× optical zoom, f=4.6~167mm
	36× optical zoom, f=4.6~167mm

	7
	Aperture
	F1.6 ~ F4.8
	F1.6 ~ F4.8

	8
	Field of View
	2.3° ~ 61.2°
	2.3° ~ 61.2°

	9
	Minimum Illumination
	Color: 0.01 Lux; B/W: 0 Lux (IR ON)
	Color: 0.01 Lux; B/W: 0 Lux (IR ON)

	10
	Day/Night
	IR-CUT auto switch
	IR-CUT auto switch

	11
	White Balance
	Auto
	Auto

	12
	Gain Control
	Auto
	Auto

	13
	Wide Dynamic
	≥80dB
	≥80dB

	14
	S/N Ratio
	≥50dB (AGC OFF)
	≥50dB (AGC OFF)

	15
	Onboard Storage
	TF card supported
	TF card supported

	16
	Electronic Shutter
	1/2 ~ 1/20,000s
	1/2 ~ 1/20,000s

	17
	Day/Night Mode
	ICR infrared filter auto switch
	ICR infrared filter auto switch

	18
	Audio Compression
	G.711, PCM
	G.711, PCM

	19
	Network Protocols
	TCP/IP, HTTP, NTP, IGMP, DHCP, UDP, SMTP, RTP, RTSP, ARP, DDNS, DNS, P2P
	TCP/IP, HTTP, NTP, IGMP, DHCP, UDP, SMTP, RTP, RTSP, ARP, DDNS, DNS, P2P

	20
	Software Compatibility
	IE, CMS, HCMS, Hikvision NVR & iVMS-4200 (V2.02.03.03+), ONVIF, Seetong Client
	IE, CMS, HCMS, Hikvision NVR & iVMS-4200 (V2.02.03.03+), ONVIF, Seetong Client

	21
	Mobile View
	Windows, Symbian, iPhone, Android via Seetong APP
	Windows, Symbian, iPhone, Android via Seetong APP

	22
	P2P
	Supported (Seetong Cloud)
	Supported (Seetong Cloud)

	23
	Presets
	128 positions
	128 positions

	24
	Cruise Groups
	8 groups
	8 groups

	25
	Guard Points
	Up to 16 points, dwell time user-selectable
	Up to 16 points, dwell time user-selectable

	26
	Pan Range
	0° ~ 360° continuous
	0° ~ 360° continuous

	27
	Tilt Range
	0° ~ 90°
	0° ~ 90°

	28
	Pan Speed
	0.1° ~ 220°/s
	0.1° ~ 220°/s

	29
	Tilt Speed
	0.1° ~ 60°/s
	0.1° ~ 60°/s

	30
	Position Display
	Supported
	Supported

	31
	IR LED Control
	PWM; 1-15 grades adjustable
	PWM; 1-15 grades adjustable

	32
	IR LEDs
	Φ42, 8-LED array
	Φ42, 8-LED array

	33
	IR Distance
	150m (night vision)
	150m (night vision)

	34
	Operating Humidity
	≤95% non-condensing
	≤95% non-condensing

	35
	Power Supply
	DC 12V ≤4A
	DC 12V ≤4A

	36
	Power Consumption
	<20W
	<20W

	37
	Operating Temperature
	Indoor: 0°C ~ +40°C; Outdoor: -40°C ~ +60°C
	Indoor: 0°C ~ +40°C; Outdoor: -40°C ~ +60°C

	38
	Surge Protection
	Instant 6000V
	Instant 6000V

	39
	Interfaces
	1× RJ45 network, power input
	1× RJ45 network, power input

	40
	Weight
	4.5 kg
	4.5 kg

	41
	Certifications
	IP66, CE, FCC, ROHS
	IP66, CE, FCC, ROHS
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Advanced Imaging Engine
2D/3D Noise Reduction & AE Exposure Algorithm
The NexPro PT736X series employs intelligent 2D and 3D noise reduction combined with an advanced auto-exposure algorithm. In low-light scenes, the image remains clean and noise-free — no muddy artifacts that plague lesser PTZs at night. The 1-15 grade adjustable IR PWM control lets integrators fine-tune illumination intensity to match the actual installation distance, preventing overexposed foreground objects while maintaining background detail.
Seamless Platform Integration
Full ONVIF 2.4 Profile S compliance guarantees plug-and-play compatibility with Hikvision NVRs and iVMS-4200 PC software (version V2.02.03.03+). The open architecture — with Linux and Windows SDK development kits plus CGI protocol — allows rapid secondary development for custom VMS platforms, access control联动, or IoT sensor integration.
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What This Means for Your Project
For Hotel Integrators: The 36× optical zoom covers expansive parking lots and entrance plazas from a single mounting point. 128 presets and 8 cruise groups allow automated patrol routes across lobby zones, pool areas, and delivery bays. The IP66 rating and -40°C to +60°C operating range mean reliable outdoor operation year-round.
For Industrial & Factory Sites: The 150-meter IR reach and 6000V surge protection handle the demands of perimeter fences, loading docks, and material storage yards. The 1-15 grade IR adjustment prevents washout at close range while maintaining long-distance visibility. P2P connectivity via Seetong Cloud enables remote inspection without complex VPN setup.
For IT Managers: An open SDK and CGI protocol allow integration into existing monitoring infrastructure without vendor lock-in. ONVIF compliance means the PTZ drops into any standards-compliant NVR environment. The dual-stream H.265+ encoding keeps bandwidth manageable even at 5MP resolution.
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© NexPro. Where Systems Connect.
Powered by Seetong Cloud & Seetong Client.
For system design assistance and PTZ integration support: contact your NexPro solutions team.


