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CCTV & SURVEILLANCE SYSTEM
NexPro 16CH 2-Bay 8MP PoE NVR (H.265+)
16 IP Channels | 16 PoE Ports | Dual HDD Bays | Seetong Cloud
PRODUCT IMAGES
	[image: NexPro 16-channel PoE NVR reference rear panel with sixteen PoE ports]

	16-Channel PoE NVR · Reference Rear Panel


Reference image shows a DC-type recorder inlet. Confirm the AC input/adapter arrangement and RCA audio connections for the final hardware configuration.
PRODUCT OVERVIEW
16-channel PoE network video recorder with 260Mbps incoming bandwidth. Supports IP camera input up to 8MP, with recording resolutions up to 5MP. Automatic camera discovery, addition and recording enable plug-and-play setup. Two SATA HDD bays support up to 14TB per HDD, with 2-channel playback and Seetong remote access.
	Product line
	CCTV & Surveillance System

	Series / family
	PoE Network Video Recorder

	Product variant
	16CH PoE NVR · 2 SATA HDD bays · Up to 8MP IP camera input

	Applications
	Small Warehouse, Restaurant, Retail


MODEL IDENTIFICATION
	Product
	Product / variant
	Channels
	Camera input
	Storage

	NexPro PoE NVR
	16CH 2-Bay 8MP PoE NVR (H.265+)
	16 IP / 16 PoE
	Up to 8MP
	2 SATA HDD bays
Max. 14TB per HDD


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Network Video Input
	16 channels

	Incoming Bandwidth
	260Mbps

	Camera Input Resolution
	Up to 8MP

	Recording Resolutions
	5MP / 4MP / 3MP / 1080P / 960P / 720P

	Video Compression
	H.265+ / H.265

	Automatic Setup
	Automatic camera discovery, addition and recording; plug-and-play setup without manual IPC addition

	Simultaneous Playback
	2 channels

	HDD Storage
	2× SATA interfaces; 2 HDD bays; up to 14TB per HDD

	Video Outputs
	1× HDMI + 1× VGA; simultaneous output supported

	Audio Output
	1× RCA

	Two-way Audio Input
	1× RCA

	LAN Interface
	1× RJ45, 10/100/1000Mbps auto-adaptive Ethernet port

	PoE Interfaces
	16× 10/100Mbps auto-adaptive Ethernet ports; 48V standard PoE supply

	USB Interfaces
	2× USB 2.0

	Network Protocols
	IPv6, UPnP, SNMP, NTP, SADP, SMTP, PPPoE, DHCP

	AC Supply
	AC 220V; 100–240V wide-range input recommended (not confirmed)

	Power Consumption
	25–30W, excluding HDDs and PoE load (reference)

	Total PoE Power Budget
	150–200W reference range; model- and PSU-dependent; final rating to be confirmed

	Operating Temperature
	-10°C to +55°C

	Weight
	Approx. 5.0kg, excluding HDDs

	Cloud and Remote Access
	Seetong Cloud; remote live view and recorded-video playback via mobile app and PC client


Power figures are reference values. The supplied 150–200W loaded-system estimate is not a verified full-load rating; confirm PSU sizing for the recorder, HDDs and maximum planned PoE load.
AI FUNCTIONS & ALARM LINKAGE
	Parameter
	Specification

	Human / Vehicle Detection
	Accurate human and vehicle detection

	Simultaneous Human Detection
	Up to 3 people detected simultaneously

	Perimeter Protection
	Tripwire detection and region intrusion detection

	NVR Alarm
	Pop-up alarm on the NVR display

	App Notifications
	Alarm push notifications, including push when the app is inactive

	Intelligent Playback
	Human and vehicle event recording playback


AI function compatibility should be confirmed with the selected IP cameras and firmware. App push notifications require an available network connection.
KEY FEATURES
1. Stable operation. 50% CPU headroom at full load, IP conflict adaptation and fault-tolerant recording with 99.99% completeness.*
2. Easy installation. Intuitive menus, IPC/router adaptation and automatic camera discovery, addition and recording for zero-configuration setup.
3. Efficient storage. H.265+ can save up to 90% of HDD space versus H.264; dual HDD bays and up to 14TB per HDD support extended recording.*
4. Fast remote access. Stated performance: 10% traffic and up to 5× smoother viewing, with rapid cloud access and remote playback.*
*Performance figures depend on test conditions and system configuration. Storage savings vary with scene and encoding settings; remote performance varies with the network.
PRODUCT FAMILY & ACCESSORY REFERENCE
	[image: NexPro PoE NVR family reference showing 4, 8 and 16 PoE ports]
	[image: Accessory reference showing an 8-port NVR chassis, power adapter, cables, mouse and small accessory packs; final 16-channel accessories depend on configuration]

	PoE NVR family · 4 / 8 / 16 ports
This datasheet covers the 16CH model only.
	Accessory reference · 8-port chassis shown
Final 16CH accessories follow the project quotation.


Accessory items shown include a power adapter, AC power cord, USB mouse, Ethernet cable and small accessory packs. Final accessory selection and quantities follow the project quotation.
APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Small Warehouse
Restaurant
Retail
	Confirm the 16CH PoE configuration, HDD capacity and AI camera compatibility.
Confirm quantity, destination, packing, branding and documentation requirements.


Project supply: MOQ — Confirm by project quantity · Lead time — Confirm by project list · FOB port — China main ports · OEM/ODM — Available; confirm project scope
PROJECT CONFIGURATION CHECKLIST
	Product configuration
	16 IP channels; 16 PoE ports; 2 SATA HDD bays; up to 14TB per HDD

	Cameras and AI functions
	Confirm IP camera models, input resolution, detection functions and alarm linkage.

	HDD and recording plan
	Confirm HDD capacity, recording mode, bitrate and required retention period.

	Interfaces and accessories
	Confirm AC input/adapter rating, RCA connections, recorder/HDD load, total PoE budget and accessories.

	Finish, branding and packing
	Confirm branding, packing and customization requirements for the order.

	Quantity and destination
	Confirm order quantity, delivery plan, destination, power plug and documentation.



STORAGE RETENTION REFERENCE (H.265+)
Actual recording storage requirements vary with the surveillance scene. The figures below are for reference only and were calculated using H.265+ encoding. All values are recording days.
	Camera
resolution
	Recording
channels
	2TB
	4TB
	6TB
	8TB
	14TB
	18TB*

	3MP
	2
	114
	228
	341
	455
	796
	1024

	
	4
	57
	114
	171
	228
	398
	512

	
	6
	38
	76
	114
	152
	265
	341

	
	8
	28
	57
	85
	114
	199
	256

	
	10
	23
	46
	68
	91
	159
	205

	4MP
	2
	102
	205
	307
	410
	717
	922

	
	4
	51
	102
	154
	205
	358
	461

	
	6
	34
	68
	102
	137
	239
	307

	
	8
	26
	51
	77
	102
	179
	230

	
	10
	20
	41
	61
	82
	143
	184

	5MP
	2
	93
	186
	279
	372
	652
	838

	
	4
	47
	93
	140
	186
	326
	419

	
	6
	31
	62
	93
	124
	217
	279

	
	8
	23
	47
	70
	93
	163
	209

	
	10
	19
	37
	56
	74
	130
	168


*The 18TB column is reproduced as a general storage reference. It does not confirm compatibility with an 18TB HDD.
HOW TO READ AND APPLY THE TABLE
Read a scenario. Select the camera resolution and recording-channel count, then read the storage-capacity column. The number is the reference duration in days.
Check project settings. The source does not specify bitrate, frame rate, recording schedule or usable-capacity allowance. Confirm these inputs when sizing storage for an installation.
Observe the source coverage. The reference covers 3MP, 4MP and 5MP at 2, 4, 6, 8 or 10 channels. No 8MP or 16-channel recording figures are provided.
APPLICATION TO THIS 16CH MODEL
	Recorder configuration
	16 IP channels; 2 SATA HDD bays; maximum 14TB per HDD

	Available source rows
	The supplied table covers 2, 4, 6, 8 and 10 recording channels. It does not include a 16-channel row.

	Full 16-channel retention
	Calculate separately using the planned recording settings and total usable HDD capacity; no 16-channel duration has been inferred here.

	Capacity scope
	The 18TB column is a general storage reference. The recorder’s specified limit remains 14TB per HDD, with two HDD bays.


Source: supplied H.265+ storage reference table. Original numerical values have been preserved.
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