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CABLE & WIRE FOR ELECTRICAL, ELV AND INDUSTRIAL PROJECTS
FLRY-B Thin-Wall Automotive Wire
Exact model: FLRY-B
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PRODUCT OVERVIEW
NexPro FLRY-B Thin-Wall Automotive Wire is supplied as a configurable automotive cable product family. Catalog models are preserved exactly as FLRY-B. Use the source-derived tables below to select the required conductor construction, core arrangement, cross-section and dimensions.
	Product line
	Cable & Wire for Electrical, ELV and Industrial Projects

	Series / family
	Automotive cable

	Exact model
	FLRY-B

	Applications
	Equipment connections, Flexible wiring, OEM electrical assemblies


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Cable category
	Catalog model
	Configuration

	FLRY-B
	FLRY-B Thin-Wall Automotive Wire
	Automotive cable
	FLRY-B
	Select from source table


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Cable category
	Automotive cable

	Catalog model
	FLRY-B

	Configuration
	Select from source table

	Manufacturer models
	FLRY-B

	Nominal Cross-section
	Conductor: No. and Dia. of Wires | Insulation: Diameter max. | Cable: Resistance at 20°C Bare/Tinned max.

	mm^2
	Conductor: No./mm | Insulation: mm | Cable: mΩ/m

	1x0.35
	Conductor: 12/0.21 | Insulation: 0.90 | Cable: 52.00/5.50

	1x0.50
	Conductor: 16/0.21 | Insulation: 1.00 | Cable: 37.10/38.20

	1x0.75
	Conductor: 24/0.21 | Insulation: 1.20 | Cable: 24.70/25.40

	1x1.00
	Conductor: 32/0.21 | Insulation: 1.35 | Cable: 18.50/19.10

	1x1.50
	Conductor: 30/0.26 | Insulation: 1.70 | Cable: 12.70/13.00

	1x2.00
	Conductor: 30/0.31 | Insulation: 1.90 | Cable: 9.31/9.59


ENGINEERING TABLES
FLRY-B · Source Specification Table 1
	Column 1
	Conductor
	Insulation
	Cable

	Nominal Cross-section
	No. and Dia. of Wires
	Diameter max.
	Resistance at 20°C Bare/Tinned max.

	mm^2
	No./mm
	mm
	mΩ/m

	1x0.35
	12/0.21
	0.90
	52.00/5.50

	1x0.50
	16/0.21
	1.00
	37.10/38.20

	1x0.75
	24/0.21
	1.20
	24.70/25.40

	1x1.00
	32/0.21
	1.35
	18.50/19.10

	1x1.50
	30/0.26
	1.70
	12.70/13.00

	1x2.00
	30/0.31
	1.90
	9.31/9.59

	1x2.50
	50/0.26
	2.20
	7.60/7.80

	1x3.00
	45/0.31
	2.40
	6.21/6.40

	1x4.00
	56/0.31
	2.75
	4.70/4.80

	1x6.00
	84/0.31
	3.30
	3.10/3.20

	1x10.00
	80/0.41
	4.50
	1.82/1.85

	1x16.00
	126/0.41
	6.30
	1.16/1.18

	1x25.00
	196/0.41
	7.80
	0.74/0.76
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