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	PRODUCT SPECIFICATION
NexPro 4MP Dual-Lens Starlight Full-Color Bullet (AI, Audio, 20W Speaker
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CCTV & SURVEILLANCE SYSTEM
NexPro 4MP Dual-Lens Starlight Full-Color Bullet (AI, Audio, 20W Speaker)
Exact model: NexPro-DL9018WZ-POE
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	NexPro-DL9018WZ-POE · Primary



PRODUCT OVERVIEW
Dual-lens fusion, Starlight full-color, Hisilicon AI, two-way audio, supports external 20W horn speaker, PoE
	Product line
	CCTV & Surveillance System

	Series / family
	Standalone model

	Exact model
	NexPro-DL9018WZ-POE

	Applications
	Perimeter, Loading Dock, Industrial, Public Space


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Resolution
	Lens 1
	Audio

	NexPro-DL9018WZ-POE
	NexPro 4MP Dual-Lens Starlight Full-Color Bullet (AI, Audio, 20W Speaker)
	4MP Dual-Lens
	F1.0 blue-wave
	20W speaker support


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Resolution
	4MP Dual-Lens

	Lens 1
	F1.0 blue-wave

	Audio
	20W speaker support; Built-in two-way intercom, supports external 20W high-power horn speaker

	Camera Type
	4MP Dual-Lens Starlight Full-Color Network Bullet Camera with PoE & External Speaker Support

	Solution
	Tianview TB53Q52

	Processor
	Hisilicon AI super-computing chip

	Image Sensor
	1/2.7″ 4MP ultra-low-light Starlight CMOS

	Lens 1 (Full-Color)
	F1.0 5MP blue-wave lens — day-like full-color at night, no motion blur

	Lens 2 (IR + Supplement)
	F1.4 5MP lens — long-range IR + smart white light, dual-light fusion

	Dual-Lens Fusion
	Combines full-color detail with IR distance for perfect night imaging

	AI Features
	Human/vehicle detection, line crossing, intrusion region

	Power
	PoE power supply

	Quotation Type
	Bulk project quotation

	OEM/ODM
	Available for selected orders

	Documents
	Datasheet and installation reference

	Category
	CCTV System


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Perimeter
Loading Dock
Industrial
Public Space
	Confirm the exact model and required configuration.
Confirm quantity, destination, packing, branding, and documentation requirements.


Project supply: MOQ — Confirm by project quantity · Lead time — Confirm by project list · FOB port — China main ports · OEM/ODM — Available; confirm project scope
PROJECT CONFIGURATION CHECKLIST
	Exact model
	NexPro-DL9018WZ-POE

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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