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CCTV & SURVEILLANCE SYSTEM
406 Series
Models: NexPro-DM406D3-4MP-TRI | NexPro-DM406D3-4MP-TRI-DJ | NexPro-DM406MQ5-5MP-TRI-DJ
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PRODUCT OVERVIEW
4MP full-color, transistor-based, 12 LEDs, built-in mic, 4000V surge protection
	Product line
	CCTV & Surveillance System

	Series / family
	406

	Exact model
	NexPro-DM406D3-4MP-TRI | NexPro-DM406D3-4MP-TRI-DJ | NexPro-DM406MQ5-5MP-TRI-DJ

	Applications
	Budget Project, Indoor Area, Corridor


MODEL COMPARISON
	Exact model
	Product / variant
	Resolution
	Lens
	Illuminator

	NexPro-DM406D3-4MP-TRI
	NexPro 4MP Cost-Effective Dual-Light Dome (12-LED, Built-in Mic)
	4MP
	F1.4 5MP fixed
	12-LED dual light

	NexPro-DM406D3-4MP-TRI-DJ
	NexPro 4MP Smart Dual-Light Dome (12-LED, Two-Way Audio & Custom Voice Alert)
	4MP (5MP sensor)
	F1.4 5MP fixed
	12-LED dual light (1W)

	NexPro-DM406MQ5-5MP-TRI-DJ
	NexPro 5MP Ultra-Bright Smart Dual-Light Dome (30-LED, Two-Way Audio & Custom Voice Alert)
	5MP
	F1.4 5MP fixed
	30-LED ultra-bright


TECHNICAL SPECIFICATIONS
	Parameter
	NexPro-DM406D3-4MP-TRI
	NexPro-DM406D3-4MP-TRI-DJ
	NexPro-DM406MQ5-5MP-TRI-DJ

	Resolution
	4MP (2560×1440) @ real-time
	4MP (5MP sensor); 4MP (2560×1440) @ real-time
	5MP (2592×1944) @ real-time

	Lens
	F1.4 5MP fixed lens
	F1.4 5MP fixed lens
	F1.4 5MP fixed lens

	Illuminator
	12-LED dual light (6×20mil IR + 6×1W warm white)
	12-LED dual light
(1W); 12-LED dual light (6×20mil IR + 6×1W warm white)
	30-LED ultra-bright dual light
(15×20mil IR + 15×0.5W warm white)

	Camera Type
	4MP Full-Color Dual-Light Network Dome Camera – Cost-Effective Series
(406 Series)
	4MP Smart Full-Color Dual-Light Network Dome Camera with Two-Way Audio & Custom Voice
(406 Series)
	5MP Ultra-Bright Smart Full-Color Dual-Light Network Dome Camera
(406 Series)

	Solution
	Tianview TR38Y33
	Tianview TB38Y51 (5MP sensor, output 4MP)
	Tianview TB38M55

	Image Sensor
	1/2.7″ 4MP CMOS, low illumination
	1/2.7″ 5MP CMOS, low illumination
	1/2.7″ 5MP CMOS, low illumination

	Lamp Board
	Transistor-based circuit design (cost-effective)
	Transistor-based circuit design
	Transistor-based circuit design

	Audio
	Built-in microphone
	Built-in microphone and speaker, two-way audio with custom voice messages
	Built-in microphone and speaker, two-way audio with custom voice messages

	Protection
	Metal front cover, 4000V lightning surge protection
	Metal front cover, front heat dissipation, 4000V surge protection
	Metal front cover, front heat dissipation, 4000V surge protection

	Light Control
	3 switchable modes
	3 switchable modes
	3 switchable modes

	Quotation Type
	Bulk project quotation
	Bulk project quotation
	Bulk project quotation

	OEM/ODM
	Available for selected orders
	Available for selected orders
	Available for selected orders

	Documents
	Datasheet and installation reference
	Datasheet and installation reference
	Datasheet and installation reference

	Category
	CCTV System
	CCTV System
	CCTV System

	Intelligent Features
	Not provided
	Customizable perimeter alert
	Intelligent perimeter alert


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Budget Project
Indoor Area
Corridor
Smart Office
Retail
Lobby
Large Warehouse
Industrial
Commercial Lobby
	Confirm the exact model and required configuration.
Confirm quantity, destination, packing, branding, and documentation requirements.


Project supply: MOQ — Confirm by project quantity · Lead time — Confirm by project list · FOB port — China main ports · OEM/ODM — Available; confirm project scope
PROJECT CONFIGURATION CHECKLIST
	Exact model
	NexPro-DM406D3-4MP-TRI

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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