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CCTV & SURVEILLANCE SYSTEM
PTL10 Series
Models: NexPro-PTL10-4MP-40X | NexPro-PTL10-5MP-25X | NexPro-PTL10-5MP-25X-FC
PRODUCT IMAGES
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PRODUCT OVERVIEW
4MP, 40x optical zoom, 7 laser IR + 11 warm LEDs, 150m illumination, AI 3-target detection, tracking, area alert, two-way audio, NVR popup, offline push
	Product line
	CCTV & Surveillance System

	Series / family
	PTL10

	Exact model
	NexPro-PTL10-4MP-40X | NexPro-PTL10-5MP-25X | NexPro-PTL10-5MP-25X-FC

	Applications
	Large Perimeter, Industrial Compound, Oil & Gas


MODEL COMPARISON
	Exact model
	Product / variant
	Resolution
	Zoom
	Illuminator

	NexPro-PTL10-4MP-40X
	NexPro 4MP 10-inch Laser Active Deterrence PTZ (40x Zoom, 150m IR, AI Tracking)
	4MP
	40x optical
	Laser IR + Warm LED

	NexPro-PTL10-5MP-25X
	NexPro 5MP 10-inch Laser PTZ (25x, 200m IR, AI Human+Vehicle Tracking, TF)
	5MP
	25x optical
	Laser 200m

	NexPro-PTL10-5MP-25X-FC
	NexPro 5MP 10-inch Full-Color Laser PTZ (25x, 200m, AI Human+Vehicle, TF)
	5MP
	25x optical
	15-laser full-color 200m


TECHNICAL SPECIFICATIONS
	Parameter
	NexPro-PTL10-4MP-40X
	NexPro-PTL10-5MP-25X
	NexPro-PTL10-5MP-25X-FC

	Resolution
	4MP
	5MP
	5MP

	Zoom
	40x optical
	25x optical
	25x optical

	Illuminator
	Laser IR + Warm LED; 7 laser IR LEDs + 11 warm white LEDs, 150m illumination
	Laser 200m; 10 laser IR + 9 warm white LEDs, 200m
	15-laser full-color 200m; 15 high-power laser warm white LEDs, 200m full-color

	Camera Type
	10-inch 4MP Laser Dual-Light Active Deterrence PTZ Camera
	10-inch 5MP Laser Dual-Light Active Deterrence PTZ with Vehicle AI
	10-inch 5MP Laser Full-Color PTZ Camera

	Solution
	Tianview Z20 platform
	Tianview customized platform
	Tianview customized platform

	Image Sensor
	4MP, H.265 encoding, 25fps
	5MP, H.265, 25fps, onboard TF card slot
	5MP, H.265, 25fps, built-in TF card

	Lens
	40x optical zoom, F1.6, 4.7mm–84.6mm
	25x optical zoom, F1.4, 5.3mm–130mm
	25x optical zoom, F1.4, 5.3mm–130mm

	AI Features
	3-target human detection, tracking, line crossing & area intrusion alert, popup, offline push
	Human & vehicle detection, tracking, line crossing, area intrusion, voice, NVR popup, offline push
	Human & vehicle detection, tracking, line crossing, area intrusion, custom voice, popup, offline push

	Audio
	External speaker support, two-way voice intercom
	External speaker support, two-way voice intercom
	External speaker support, two-way intercom

	Alarm
	NVR popup alert, offline mobile push
	NVR popup, offline push
	NVR popup, offline push

	Quotation Type
	Bulk project quotation
	Bulk project quotation
	Bulk project quotation

	OEM/ODM
	Available for selected orders
	Available for selected orders
	Available for selected orders

	Documents
	Datasheet and installation reference
	Datasheet and installation reference
	Datasheet and installation reference

	Category
	CCTV System
	CCTV System
	CCTV System


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Large Perimeter
Industrial Compound
Oil & Gas
Critical Infrastructure
Oil Depot
Logistics Hub
Forensic Perimeter
Port
	Confirm the exact model and required configuration.
Confirm quantity, destination, packing, branding, and documentation requirements.


Project supply: MOQ — Confirm by project quantity · Lead time — Confirm by project list · FOB port — China main ports · OEM/ODM — Available; confirm project scope
PROJECT CONFIGURATION CHECKLIST
	Exact model
	NexPro-PTL10-4MP-40X

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
	Page 1


image2.png




image3.png




image1.png








