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	PRODUCT SPECIFICATION
NexPro 5MP High-Altitude Object Detection Camera (Built-in Algorithm)
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CCTV & SURVEILLANCE SYSTEM
NexPro 5MP High-Altitude Object Detection Camera (Built-in Algorithm)
Exact model: NexPro-SC1040M15-GK
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PRODUCT OVERVIEW
5MP, built-in falling object trajectory algorithm, dedicated for high-rise littering surveillance
	Product line
	CCTV & Surveillance System

	Series / family
	Standalone model

	Exact model
	NexPro-SC1040M15-GK

	Applications
	Residential Tower, Commercial High-Rise, Property Management


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Resolution
	Algorithm
	Use Case

	NexPro-SC1040M15-GK
	NexPro 5MP High-Altitude Object Detection Camera (Built-in Algorithm)
	5MP
	Built-in trajectory
	High-rise anti-littering


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Resolution
	5MP

	Algorithm
	Built-in trajectory

	Use Case
	High-rise anti-littering

	Camera Type
	5MP High-Altitude Object Detection Network Camera

	Solution
	SSC30KD + SmartSens SC500AI

	Image Sensor
	1/2.7″ 5MP CMOS, H.265 encoding

	Special Feature
	Built-in object falling trajectory algorithm for high-rise littering and falling object monitoring

	Application
	Residential and commercial high-rise perimeters

	Quotation Type
	Bulk project quotation

	OEM/ODM
	Available for selected orders

	Documents
	Datasheet and installation reference

	Category
	CCTV System


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Residential Tower
Commercial High-Rise
Property Management
	Confirm the exact model and required configuration.
Confirm quantity, destination, packing, branding, and documentation requirements.


Project supply: MOQ — Confirm by project quantity · Lead time — Confirm by project list · FOB port — China main ports · OEM/ODM — Available; confirm project scope
PROJECT CONFIGURATION CHECKLIST
	Exact model
	NexPro-SC1040M15-GK

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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