
	[image: ]
	PRODUCT SPECIFICATION
16-Port Remote IP KVM Series


[image: ]
RACK KVM & REMOTE CONSOLE MANAGEMENT
16-Port Remote IP KVM Series
Models: SP5716 | SP5916
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PRODUCT OVERVIEW
16-port IP KVM consoles for local and remote server management.
	Product line
	Rack KVM & Remote Console Management

	Series / family
	kvm-ip16

	Exact model
	SP5716 | SP5916

	Applications
	Remote server access, Data center operations, Network equipment rooms


MODEL COMPARISON
	Exact model
	Product / variant
	Port Count
	Resolution
	Dimensions

	SP5716
	SP5716 16-port remote IP KVM
	16
	1280 × 1024
	485 × 570 × 44 mm

	SP5916
	SP5916 16-Port Remote IP KVM, 600 mm Depth
	16
	1280 × 1024
	485 × 600 × 44 mm


TECHNICAL SPECIFICATIONS
	Parameter
	SP5716
	SP5916

	Port Count
	16
	16

	Resolution
	1280 × 1024
	1280 × 1024

	Dimensions
	485 × 570 × 44 mm
	485 × 600 × 44 mm

	Maximum Cascade Capacity
	Up to 256 devices
Source catalog wording:  “connections 256”
	Up to 256 devices
Source catalog wording:  “connections 256”

	I/O Interface
	PS/2 / USB dual-interface converter module
	PS/2 / USB dual-interface converter module

	Scan Interval
	1–255 seconds
	1–255 seconds

	System Compatibility
	Windows, Vista, Linux, etc.
	Windows, Vista, Linux, etc.

	Power Input
	A C100-240V, 50-60Hz, 1 A
	A C100-240V, 50-60Hz, 1 A

	Power Consumption
	120V at 23 W; 230V at 25 W
	120V at 23 W; 230V at 25 W

	Operating Temperature
	0-40℃
	0-40℃

	Storage Temperature
	-20-60℃
	-20-60℃

	Humidity
	0-80%RH, non-condensing
	0-80%RH, non-condensing

	Warranty
	3 years for main unit; 1 year for display
	3 years for main unit; 1 year for display

	Product series
	16-Port Remote IP KVM Series
	16-Port Remote IP KVM Series

	Product category
	KVM
	KVM


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Remote server access
Data center operations
Network equipment rooms
	Confirm the application, rack or room position, destination-market interface and mounting requirement.
Confirm electrical, network, accessory or protection scope from the product family and project drawings.
Confirm quantity, labeling, packing and required documents before purchase order.


Project supply: MOQ — Confirm by model and project quantity · Lead time — Confirm after configuration review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	SP5716

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
	Page 1


image2.png




image3.jpg




image4.jpg
External m:ouse and
keyboard

External display





image5.jpg




image6.jpg




image1.png








