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RACK KVM & REMOTE CONSOLE MANAGEMENT
SP8032 16-Port Digital KVM
Exact model: SP8032
PRODUCT IMAGES
	[image: ]
	[image: ]

	SP8032 · Primary
	SP8032 · Gallery



PRODUCT OVERVIEW
2 documented configurations are consolidated on this product-group page so buyers can compare specifications without duplicate catalog cards.
	Product line
	Rack KVM & Remote Console Management

	Series / family
	kvm-sp8032

	Exact model
	SP8032

	Applications
	Server rack management, Data center operations, Remote equipment maintenance


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Configurations
	Server Ports
	Network Port

	SP8032
	SP8032 16-Port Digital KVM
	2
	16
	RJ45


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Configurations
	2

	Server Ports
	16

	Network Port
	RJ45

	Resolution
	1920 × 1200px

	Supported Systems
	Windows, Linux, Mac, Sun, etc.

	Power
	60 W

	Dimensions
	400 × 440 × 44 mm

	Installation
	19-inch standard rack cabinet

	Transmission Distance
	50 m

	Weight
	6.6kg

	User Configuration
	1 local user + 2 remote users

	Product series
	SP8032 16-Port Digital KVM

	Entity type
	Product group with selectable configurations


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Server rack management
Data center operations
Remote equipment maintenance
	Confirm the application, rack or room position, destination-market interface and mounting requirement.
Confirm electrical, network, accessory or protection scope from the product family and project drawings.
Confirm quantity, labeling, packing and required documents before purchase order.


Project supply: MOQ — Confirm by model and project quantity · Lead time — Confirm after configuration review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	SP8032

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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