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RACK PDU & POWER DISTRIBUTION
DS8118 Hardwired 8-Outlet New Chinese-Standard PDU
Exact model: DS8118
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PRODUCT OVERVIEW
High-power and special-input/output rack PDU configurations for project-specific power distribution.
	Product line
	Rack PDU & Power Distribution

	Series / family
	pdu-special

	Exact model
	DS8118

	Applications
	Special-input equipment racks, High-load cabinets, Project-configured power distribution


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Input Method
	Input Current
	Rated Load

	DS8118
	DS8118 Hardwired 8-Outlet New Chinese-Standard PDU
	No input cable; terminal-block / hardwired input
	16 A
	4000 W


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Input Method
	No input cable; terminal-block / hardwired input

	Input Current
	16 A

	Rated Load
	4000 W

	Function Module
	Switch protection

	Output
	8 × 10 A new Chinese-standard outlets

	Dimensions
	485 × 44.5 × 44.5 mm

	Product series
	High-Power & Special I/O PDU Series

	Product category
	PDU


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Special-input equipment racks
High-load cabinets
Project-configured power distribution
	Confirm the application, rack or room position, destination-market interface and mounting requirement.
Confirm electrical, network, accessory or protection scope from the product family and project drawings.
Confirm quantity, labeling, packing and required documents before purchase order.


Project supply: MOQ — Confirm by model and project quantity · Lead time — Confirm after configuration review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	DS8118

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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