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RACK PDU & POWER DISTRIBUTION
High-Power & Special I/O PDU Series
Models: DS8118 | SP51104 | SP5281 | SP9041S
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PRODUCT OVERVIEW
High-power and special-input/output rack PDU configurations for project-specific power distribution.
	Product line
	Rack PDU & Power Distribution

	Series / family
	pdu-special

	Exact model
	DS8118 | SP51104 | SP5281 | SP9041S

	Applications
	Special-input equipment racks, High-load cabinets, Project-configured power distribution


MODEL COMPARISON
	Exact model
	Product / variant
	Input Current
	Input Cable
	Input Method

	DS8118
	DS8118 Hardwired 8-Outlet New Chinese-Standard PDU
	16 A
	Not provided
	No input cable; terminal-block / hardwired input

	SP51104
	SP51104 High-Power & Special I/O PDU
	16 A
	3 m, 2.5 mm²
	Not provided

	SP5281
	SP5281 16 A Universal-Outlet PDU
	16 A
	3 m, 2.5 mm²
	Not provided

	SP9041S
	SP9041S 4-Outlet 16 A High-Power Terminal-Block PDU
	32 A
	Not provided
	Not provided


TECHNICAL SPECIFICATIONS
	Parameter
	DS8118
	SP51104
	SP5281
	SP9041S

	Input Method
	No input cable; terminal-block / hardwired input
	Not provided
	Not provided
	Not provided

	Input Current
	16 A
	16 A
	16 A
	32 A

	Rated Load — Key Specifications
	4000 W
	Not provided
	Not provided
	Not provided

	Function Module — Source Technical Data
	Switch protection
	Power indicator
	Switch protection
	Not provided

	Output — Source Technical Data
	8 × 10 A new Chinese-standard outlets
	10 × 10 A universal outlets
	8 × 16 A universal outlets
	Not provided

	Dimensions
	485 × 44.5 × 44.5 mm
	485 × 44.5 × 44.5 mm
	485 × 44.5 × 44.5 mm
	485 × 44.5 × 44.5 mm

	Product series
	High-Power & Special I/O PDU Series
	High-Power & Special I/O PDU Series
	High-Power & Special I/O PDU Series
	High-Power & Special I/O PDU Series

	Product category
	PDU
	Not provided
	PDU
	PDU

	Configurations
	Not provided
	2
	Not provided
	Not provided

	Input Cable
	Not provided
	3 m, 2.5 mm²
	3 m, 2.5 mm²
	Not provided

	Input Plug — Source Technical Data
	Not provided
	16A Chinese-standard plug
	Not provided
	Not provided

	Rated Load — Source Technical Data
	Not provided
	4000 W
	4000 W
	8000 W

	Entity type
	Not provided
	Product group with selectable configurations
	Not provided
	Not provided

	Input Plug — Key Specifications
	Not provided
	Not provided
	16A Chinese-standard plug
	Not provided

	Function Module — Key Specifications
	Not provided
	Not provided
	Not provided
	Junction box / terminal block

	Output — Key Specifications
	Not provided
	Not provided
	Not provided
	4 × 16 A Chinese-standard outlets


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Special-input equipment racks
High-load cabinets
Project-configured power distribution
	Confirm the application, rack or room position, destination-market interface and mounting requirement.
Confirm electrical, network, accessory or protection scope from the product family and project drawings.
Confirm quantity, labeling, packing and required documents before purchase order.


Project supply: MOQ — Confirm by model and project quantity · Lead time — Confirm after configuration review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	DS8118

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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