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RACK PDU & POWER DISTRIBUTION
Metered PDU Series
Models: SP5086 | SP5186
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PRODUCT OVERVIEW
Rack PDU with local voltage and current display for basic load monitoring.
	Product line
	Rack PDU & Power Distribution

	Series / family
	pdu-metered

	Exact model
	SP5086 | SP5186

	Applications
	Server racks, Network rooms, Load monitoring projects


MODEL COMPARISON
	Exact model
	Product / variant
	Input Current
	Cable Specification
	Rated Load

	SP5086
	SP5086 16Ametered PDU
	16 A
	3 × 2.5 mm²
	4000 W

	SP5186
	SP5186 16Ametered PDU
	16 A
	Not provided
	Not provided


TECHNICAL SPECIFICATIONS
	Parameter
	SP5086
	SP5186

	Cable Specification
	3 × 2.5 mm²
	Not provided

	Input Current
	16 A
	16 A

	Rated Load — Key Specifications
	4000 W
	Not provided

	Input Plug — Source Technical Data
	16A Chinese-standard plug
	Not provided

	Function Module
	Current and voltage display
	Current and voltage display

	Output
	8 × 16 A Chinese-standard outlets
	8 × 10 A universal outlets

	Dimensions
	485 × 44.5 × 44.5 mm
	485 × 44.5 × 44.5 mm

	Product series
	Metered PDU Series
	Metered PDU Series

	Product category
	PDU
	PDU

	Input Cable
	Not provided
	3 m, 2.5 mm²

	Input Plug — Key Specifications
	Not provided
	16A Chinese-standard plug

	Rated Load — Source Technical Data
	Not provided
	4000 W


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Server racks
Network rooms
Load monitoring projects
	Confirm the application, rack or room position, destination-market interface and mounting requirement.
Confirm electrical, network, accessory or protection scope from the product family and project drawings.
Confirm quantity, labeling, packing and required documents before purchase order.


Project supply: MOQ — Confirm by model and project quantity · Lead time — Confirm after configuration review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	SP5086

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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