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RACK CABINETS & DATA CENTER CONTAINMENT
K1-6638 38U K1 network cabinet
Exact model: K1-6638
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PRODUCT OVERVIEW
19-inch network and server cabinets for standard IT, networking and security equipment.
	Product line
	Rack Cabinets & Data Center Containment

	Series / family
	k1

	Exact model
	K1-6638

	Applications
	Wall-mount network cabinets, CCTV and ELV equipment racks, Small server rooms


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Type
	Dimensions
	Height

	K1-6638
	K1-6638 38U K1 network cabinet
	Network cabinet
	600 × 600 × 1800 mm
	38U


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Type
	Network cabinet

	Dimensions
	600 × 600 × 1800 mm

	Height
	38U

	Mounting Rail Spacing
	485 mm (19-inch standard)

	Sheet Thickness
	mounting rails 2.0 mm; other panels 1.1 mm

	Material / Finish
	SPCC cold-rolled steel, degreased and powder-coated

	Series Load Capacity
	≤600kg

	Standard Configuration
	PDU × 1、cage nuts and screws × 20、M12leveling feet × 4、38Umounting rails × 4、front and rear mesh doors × 1、side panels × 2、fans × 1、shelves × 3、casters × 4

	Recommended Equipment Depth
	<450 mm

	Product series
	K1 Network & Server Cabinet Series

	Product category
	Data Center Cabinet


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Wall-mount network cabinets
CCTV and ELV equipment racks
Small server rooms
	Confirm the application, rack or room position, destination-market interface and mounting requirement.
Confirm electrical, network, accessory or protection scope from the product family and project drawings.
Confirm quantity, labeling, packing and required documents before purchase order.


Project supply: MOQ — Confirm by model and project quantity · Lead time — Confirm after configuration review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	K1-6638

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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