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RACK CABINETS & DATA CENTER CONTAINMENT
K2 Network Cabinet Series
Models: K2-6620 | K2-6622
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PRODUCT OVERVIEW
19-inch network cabinets for medium-capacity equipment installation.
	Product line
	Rack Cabinets & Data Center Containment

	Series / family
	k2

	Exact model
	K2-6620 | K2-6622

	Applications
	Network rooms, ELV equipment cabinets, Structured cabling racks


MODEL COMPARISON
	Exact model
	Product / variant
	Type
	Dimensions
	Height

	K2-6620
	K2-6620 20U K2 network cabinet
	Network cabinet
	600 × 600 × 1000 mm
	20U

	K2-6622
	K2-6622 22U K2 network cabinet
	Network cabinet
	600 × 600 × 1200 mm
	22U


TECHNICAL SPECIFICATIONS
	Parameter
	K2-6620
	K2-6622

	Type
	Network cabinet
	Network cabinet

	Dimensions
	600 × 600 × 1000 mm
	600 × 600 × 1200 mm

	Height
	20U
	22U

	Mounting Rail Spacing
	485 mm (19-inch standard)
	485 mm (19-inch standard)

	Sheet Thickness
	mounting rails 2.0 mm; other panels 1.0 mm
	mounting rails 2.0 mm; other panels 1.0 mm

	Material / Finish
	SPCC cold-rolled steel, degreased and powder-coated
	SPCC cold-rolled steel, degreased and powder-coated

	Series Load Capacity
	≤400kg
	≤400kg

	Standard Configuration
	PDU × 1、cage nuts and screws × 20、M12leveling feet × 4、20Umounting rails × 4、front and rear mesh doors × 1、side panels × 2、fans × 1、shelves × 1、casters × 4
	PDU × 1、cage nuts and screws × 20、M12leveling feet × 4、22Umounting rails × 4、front and rear mesh doors × 1、side panels × 2、fans × 1、shelves × 1、casters × 4

	Recommended Equipment Depth
	<450 mm
	<450 mm

	Product series
	K2 Network Cabinet Series
	K2 Network Cabinet Series

	Product category
	Data Center Cabinet
	Data Center Cabinet


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Network rooms
ELV equipment cabinets
Structured cabling racks
	Confirm the application, rack or room position, destination-market interface and mounting requirement.
Confirm electrical, network, accessory or protection scope from the product family and project drawings.
Confirm quantity, labeling, packing and required documents before purchase order.


Project supply: MOQ — Confirm by model and project quantity · Lead time — Confirm after configuration review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	K2-6620

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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