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RACK CABINETS & DATA CENTER CONTAINMENT
KP-C Electromagnetic Shielding Cabinet Series
Exact model: KP-C
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PRODUCT OVERVIEW
14 documented configurations are consolidated on this product-group page so buyers can compare specifications without duplicate catalog cards.
	Product line
	Rack Cabinets & Data Center Containment

	Series / family
	shielding

	Exact model
	KP-C

	Applications
	EMI-sensitive equipment rooms, Data rooms, Security and communication cabinets


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Configurations
	Rack Height
	Net Weight

	KP-C
	KP-C Electromagnetic Shielding Cabinet Series
	14
	10U
	100kg


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Configurations
	14

	Rack Height
	10U

	Net Weight
	100kg

	Overall Dimensions
	700 × 980 × 800 mm

	Standard Configuration
	10 network-cable waveguides; 5 fiber waveguides; 1 × 16 A filter; 2–3 shelves; 1 × 16 A 6-outlet PDU; 4 adjustable fans; 2 ventilation waveguide windows
(catalog: 300 × 30 type)

	Optional Configuration
	Humidity monitoring, alarm display, combination lock, fingerprint access, four fan groups / high-power fans, waveguide window, opening rear door, air-conditioner extension, air duct, top cable entry, filter, PDU and other options

	Product series
	KP-C Electromagnetic Shielding Cabinet Series

	Entity type
	Product group with selectable configurations


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	EMI-sensitive equipment rooms
Data rooms
Security and communication cabinets
	Confirm the application, rack or room position, destination-market interface and mounting requirement.
Confirm electrical, network, accessory or protection scope from the product family and project drawings.
Confirm quantity, labeling, packing and required documents before purchase order.


Project supply: MOQ — Confirm by model and project quantity · Lead time — Confirm after configuration review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	KP-C

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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