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	PRODUCT SPECIFICATION
86-Type Information Faceplate Series


[image: ]
PATCH PANELS, FACEPLATES & KEYSTONE MODULES
86-Type Information Faceplate Series
Models: SP8601 | SP8602 | SP8604
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PRODUCT OVERVIEW
86 × 86 mm information faceplates for modular network and voice outlets.
	Product line
	Patch Panels, Faceplates & Keystone Modules

	Series / family
	faceplate

	Exact model
	SP8601 | SP8602 | SP8604

	Applications
	Office network outlets, ELV cabling projects, Wall-mounted data points


MODEL COMPARISON
	Exact model
	Product / variant
	Specification
	Material
	Application Environment

	SP8601
	SP8601 86-Type 1-Port Network Faceplate
	1-port faceplate
	Flame-retardant PC
	Home, internet cafe, office and similar installations

	SP8602
	SP8602 86-Type 2-Port Network Faceplate
	2-port faceplate
	Flame-retardant PC
	Home, internet cafe, office and similar installations

	SP8604
	SP8604 86-Type 4-Port Network Faceplate
	4-port faceplate
	Flame-retardant PC
	Home, internet cafe, office and similar installations


TECHNICAL SPECIFICATIONS
	Parameter
	SP8601
	SP8602
	SP8604

	Specification
	1-port faceplate
	2-port faceplate
	4-port faceplate

	Material
	Flame-retardant PC
	Flame-retardant PC
	Flame-retardant PC

	Application Environment
	Home, internet cafe, office and similar installations
	Home, internet cafe, office and similar installations
	Home, internet cafe, office and similar installations

	Dimensions
	86 × 86 mm
	86 × 86 mm
	86 × 86 mm

	Mounting Hole Spacing
	60 mm
	60 mm
	60 mm

	Product series
	86-Type Information Faceplate Series
	86-Type Information Faceplate Series
	86-Type Information Faceplate Series

	Product category
	Structured Cabling Accessory
	Structured Cabling Accessory
	Structured Cabling Accessory


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	Office network outlets
ELV cabling projects
Wall-mounted data points
	Confirm the application, rack or room position, destination-market interface and mounting requirement.
Confirm electrical, network, accessory or protection scope from the product family and project drawings.
Confirm quantity, labeling, packing and required documents before purchase order.


Project supply: MOQ — Confirm by model and project quantity · Lead time — Confirm after configuration review · FOB port — Confirm in project quotation · OEM/ODM — To be confirmed
PROJECT CONFIGURATION CHECKLIST
	Exact model
	SP8601

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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