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UPS UNINTERRUPTIBLE POWER SUPPLY
FPS-500 Portable Power Station
Exact model: FPS-500-PORTABLE-POWER-STATION
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PRODUCT OVERVIEW
FPS-500 Portable Power Station with 1 source-reviewed model for Emergency response, field work, temporary offices and mobile equipment. Model configuration and destination-market requirements are confirmed during RFQ review.
	Product line
	UPS Uninterruptible Power Supply

	Series / family
	Standalone model

	Exact model
	FPS-500-PORTABLE-POWER-STATION

	Applications
	Emergency response, field work, temporary offices and mobile equipment


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Topology
	Power Range
	Phase

	FPS-500-PORTABLE-POWER-STATION
	FPS-500 Portable Power Station
	Portable energy storage power station
	500W / 230Wh
	AC and solar charging input / AC and DC output


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Topology
	Portable energy storage power station

	Power Range
	500W / 230Wh

	Phase
	AC and solar charging input / AC and DC output

	Form Factor
	Portable

	Waveform
	Modified sine wave

	Power Factor
	Model-specific; confirm on quotation

	Battery Types
	Source-defined lithium or LiFePO4 configuration

	SKU
	FPS-500-PORTABLE-POWER-STATION

	Available Configurations
	FPS-500

	Exact Configuration
	Confirm one listed configuration during RFQ review

	Destination Requirements
	To be confirmed


ENGINEERING TABLES
FPS-500-PORTABLE-POWER-STATION · Complete Model Specifications — FPS-500
	Parameter
	FPS-500

	Rated capacity
	500W / 230Wh

	Battery configuration
	Not provided

	Dimensions
	317*107*175mm

	Net weight
	5.1KG

	Transfer time
	Not provided

	Efficiency
	Not provided

	Model configuration — Rated capacity
	500W / 230Wh

	Model configuration — Product dimensions
	317*107*175mm

	Model configuration — Net weight
	5.1KG

	AC Output — Output Voltage
	220VAC

	AC Output — Max Power
	500W

	AC Output — Wave Form
	Modified Sine Wave

	AC Output — Frequency
	50Hz/60HZ

	DC Output — USB
	4PCS USB output 5V/3A(total current)

	DC Output — DC
	2PCS DC5.5/2.1 output 12V/5A(total current) (Option)

	Input — AC Input
	INV mode 70~145VAC OR 140 ~260VAC

	Input — AC AC Charging
	4hours

	Input — Solar Charging
	Standard 5A

	Input — Car Charging
	14.6V/4A(Option)

	Battery — Capacity
	Standard 230WH 12.8V/18AH

	Battery — Battery type
	LiFePO4 battery

	PHYSICAL — Size /(mm)
	317*107*175mm

	PHYSICAL — Net weight
	5.1KG

	PHYSICAL — Size/CTN(mm)
	380*359*488

	PHYSICAL — Gross (KG)
	23.8

	PHYSICAL — PCS per CTN
	4



	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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