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UPS UNINTERRUPTIBLE POWER SUPPLY
IFR 48V Rack-Mounted LiFePO4 Battery
Exact model: NX-UP-BA-003
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PRODUCT OVERVIEW
IFR 48V Rack-Mounted LiFePO4 Battery with 1 source-reviewed model for UPS DC backup, telecom backup and residential energy storage. Model configuration and destination-market requirements are confirmed during RFQ review.
	Product line
	UPS Uninterruptible Power Supply

	Series / family
	Standalone model

	Exact model
	NX-UP-BA-003

	Applications
	UPS DC backup, telecom backup and residential energy storage


MODEL IDENTIFICATION
	Exact model
	Product / variant
	Topology
	Power
	Phase

	NX-UP-BA-003
	IFR 48V Rack-Mounted LiFePO4 Battery
	48V rack-mounted LiFePO4 battery
	48V / 200Ah / 9.6kWh
	DC discharge


TECHNICAL SPECIFICATIONS
	Parameter
	Specification

	Topology
	48V rack-mounted LiFePO4 battery

	Power
	48V / 200Ah / 9.6kWh

	Phase
	DC charge / DC discharge

	SKU
	NX-UP-BA-003

	Power Range
	48V / 200Ah / 9.6kWh

	Waveform
	DC

	Power Factor
	Model-specific; confirm on quotation

	Quotation Type
	Bulk project quotation

	OEM/ODM
	Available

	Documents
	Datasheet and installation reference

	Category
	UPS Power


APPLICATIONS & RFQ CONFIRMATION
	Typical applications
	Confirm in the project RFQ

	UPS DC backup
telecom backup and residential energy storage
	Confirm the exact model and required configuration.
Confirm quantity, destination, packing, branding, and documentation requirements.


Project supply: MOQ — Confirm by project quantity · Lead time — Confirm by project list · FOB port — China main ports · OEM/ODM — Available; confirm project scope
PROJECT CONFIGURATION CHECKLIST
	Exact model
	NX-UP-BA-003

	Application and site conditions
	Confirm installation environment and operating requirements.

	Quantity and model mix
	Confirm forecast quantity, phase plan and required variants.

	Interfaces and accessories
	Confirm compatible interfaces, accessories and system integration scope.

	Finish, branding and packing
	Confirm only when project customization is required.

	Documentation and destination
	Confirm drawings, datasheets, packing documents and destination country or port.
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	NexPro Product Intelligence
	Confirm final configuration in the project RFQ
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